{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet2"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet2","index":0,"n_rows":972,"n_cols":6,"rows_kept":972,"merged":[[0,0,0,5],[2,0,2,5],[3,1,3,2],[49,1,49,2],[104,1,104,2],[121,1,121,2],[165,1,165,3],[166,1,166,2],[241,1,241,2],[410,1,410,2],[593,1,593,2],[659,1,659,3],[864,1,864,3],[891,1,891,3],[954,1,954,3],[968,1,968,5],[969,1,969,5],[970,1,970,5],[971,1,971,5]]}
["泸州市中医医院维修物资及工器具采购明细报价表"]
["序号","名称","规格型号（实质性要求）","技术参数（实质性要求）","单位","投标单价（元）"]
["1、水工类"]
[null,"管道、管件类"]
[1,"PPR热水管","Φ20","壁厚≥2.8mm/压力等级：S3.2/材质：聚丙烯/符合：GB/T18742.1-2017 GB/T18742.2-2017/颜色综合","根（4米）"]
[2,"PPR热熔管件(XX)","Φ20","含直接、弯头、过桥、三通、变截等，壁厚≥2.8mm/压力等级S3.2/材质：聚丙烯/符合：GB/T18742.1-2017 GB/T18742.2-2017/颜色综合","个"]
[3,"PPR带丝管件(XX)","Φ20","含直接/、弯头、三通、变截等，壁厚≥2.8mm/压力等级：S3.2/材质：聚丙烯/符合：GB/T18742.1-2017 GB/T18742.2-2017/颜色综合","个"]
[4,"PPR热水管","Φ25","壁厚≥3.5mm/压力等级：S3.2/材质：聚丙烯/符合：GB/T18742.1-2017 GB/T18742.2-2017/颜色综合","根（4米）"]
[5,"PPR热熔管件(XX)","Φ25","含直接、弯头、过桥、三通、变截等，壁厚≥3.5mm/压力等级S3.2/材质：聚丙烯/符合：GB/T18742.1-2017 GB/T18742.2-2017/颜色综合","个"]
[6,"PPR带丝管件(XX)","Φ25","含直接/、弯头、三通、变截等，壁厚≥3.5mm/压力等级：S3.2/材质：聚丙烯/符合：GB/T18742.1-2017 GB/T18742.2-2017/颜色综合","个"]
[7,"PPR热水管","Φ32","壁厚≥4.4mm/压力等级：S3.2/材质：聚丙烯/符合：GB/T18742.1-2017 GB/T18742.2-2017/颜色综合","根（4米）"]
[8,"PPR热熔管件(XX)","Φ32","含直接、弯头、过桥、三通、变截等，壁厚≥4.4mm/压力等级：S3.2/材质：聚丙烯/符合：GB/T18742.1-2017 GB/T18742.2-2017/颜色综合","个"]
[9,"PPR带丝管件(XX)","Φ32","含直接、弯头、三通、变截等，壁厚≥4.4mm/压力等级：S3.2/材质：聚丙烯/符合：GB/T18742.1-2017 GB/T18742.2-2017/颜色综合","个"]
[10,"PPR热水管","Φ50","壁厚≥6.9mm/压力等级：S3.2/材质：聚丙烯/符合：GB/T18742.1-2017 GB/T18742.2-2017/颜色综合","根（4米）"]
[11,"PPR热熔管件(XX)","Φ50","含直接、弯头、过桥、三通、变截等，壁厚≥6.9mm/压力等级：S3.2/材质：聚丙烯/符合：GB/T18742.1-2017 GB/T18742.2-2017/颜色综合","个"]
[12,"PPR带丝管件(XX)","Φ50","含直接、弯头、三通、变截等，壁厚≥6.9mm/压力等级：S3.2/材质：聚丙烯/符合：GB/T18742.1-2017 GB/T18742.2-2017/颜色综合","个"]
[13,"PPR热水管","Φ63","壁厚≥8.6mm/压力等级：S3.2/材质：聚丙烯/符合：GB/T18742.1-2017 GB/T18742.2-2017/颜色综合","根（4米）"]
[14,"PPR热熔管件(XX)","Φ63","含直接、弯头、过桥、三通、变截等，壁厚≥8.6mm/压力等级：S3.2/材质：聚丙烯/符合：GB/T18742.1-2017 GB/T18742.2-2017/颜色综合","个"]
[15,"PPR带丝管件(XX)","Φ63","含直接、弯头、三通、变截等，壁厚≥8.6mm/压力等级：S3.2/材质：聚丙烯/符合：GB/T18742.1-2017 GB/T18742.2-2017/颜色综合","个"]
[16,"黄铜带丝管件(XX)","Φ15-20","含直接、弯头、变截等","个"]
[17,"黄铜带丝管件","Φ15-20","三通","个"]
[18,"黄铜带丝管件(XX)","Φ25-32","含直接、弯头、变截等","个"]
[19,"黄铜带丝管件","Φ25-32","三通","个"]
[20,"黄铜带丝管件(XX)","Φ50","含直接、弯头、变截等","个"]
[21,"黄铜带丝管件","Φ50","三通","个"]
[22,"黄铜带丝管件(XX)","Φ63","含直接、弯头、变截等","个"]
[23,"黄铜带丝管件","Φ63","三通","个"]
[24,"PVC-U排水管","Φ20","厚度≥1.8mm/无铅/符合：GB/T 5836.1-2018","根（4米）"]
[25,"PVC-U排水管","Φ25","厚度≥2.0mm/无铅/符合：GB/T 5836.1-2018","根（4米）"]
[26,"PVC-U排水管","Φ32","厚度≥2.0mm/无铅/符合：GB/T 5836.1-2018","根（4米）"]
[27,"PVC-U排水管","Φ40","厚度≥2.0mm/无铅/符合：GB/T 5836.1-2018","根（4米）"]
[28,"PVC-U排水管","Φ50","厚度≥2.0mm/无铅/符合：GB/T 5836.1-2018","根（4米）"]
[29,"PVC-U排水管","Φ75","厚度≥2.3mm/无铅/符合：GB/T 5836.1-2018","根（4米）"]
[30,"PVC-U排水管","Φ110","厚度≥3.2mm/无铅/符合：GB/T 5836.1-2018","根（4米）"]
[31,"PVC-U排水管","Φ160","厚度≥4mm/无铅/符合：GB/T 5836.1-2018","根（4米）"]
[32,"PVC-U排水管件","DN20-25","包括直接、弯头、三通、过桥、抢修节、各类存水弯等/无铅/符合：GB/T 5836.1-2018","个"]
[33,"PVC-U排水管件","DN32-50","包括直接、弯头、三通、过桥、抢修节、各类存水弯等/无铅/符合：GB/T 5836.1-2018","个"]
[34,"PVC-U排水管件","DN75","包括直接、弯头、三通、过桥、抢修节、各类存水弯等/无铅/符合：GB/T 5836.1-2018","个"]
[35,"PVC-U排水管件","DN110","包括直接、弯头、三通、过桥、抢修节、各类存水弯等/无铅/符合：GB/T 5836.1-2018","个"]
[36,"PVC-U排水管件","DN160","包括直接、弯头、三通、过桥、抢修节、各类存水弯等/无铅/符合：GB/T 5836.1-2018","个"]
[37,"PVC管卡","Φ25","含可根据实际需求选择底座、连接杆、螺栓、钉子、膨胀螺栓等配件，厚度≥3.2mm，,宽度≥15mm","个"]
[38,"PVC管卡","Φ32","含可根据实际需求选择底座、连接杆、螺栓、钉子、膨胀螺栓等配件，厚度≥4.8mm，,宽度≥15mm","个"]
[39,"PVC管卡","Φ50","含可根据实际需求选择底座、连接杆、螺栓、钉子、膨胀螺栓等配件，厚度≥4.8mm，,宽度≥15mm","个"]
[40,"PVC管卡","Φ75","含可根据实际需求选择底座、连接杆、螺栓、钉子、膨胀螺栓等配件，厚度≥4.8mm，,宽度≥15mm","个"]
[41,"PVC管卡","Φ110","含可根据实际需求选择底座、连接杆、螺栓、钉子、膨胀螺栓等配件，厚度≥5.9mm，,宽度≥20mm","个"]
[42,"排水软管","Φ20","厚型/符合GB/T 19472.1-2019","米"]
[43,"排水软管","Φ25","厚型/符合GB/T 19472.1-2019","米"]
[44,"塑料蹲便器水箱冲水管","综合","包含可选择胶垫、连接件、转换头等配件/厚度≥2mm","根"]
[45,"空调排水管","通用","聚乙烯管身（内层加入炭黑），接口直径15-20mm","米"]
[46,"阀门、开关类"]
[47,"PPR闸阀","DN20","壁厚≥3.5mm/压力等级：S3.2/材质：聚丙烯/符合：GB/T18742.1-2017 GB/T18742.2-2017/颜色综合","个"]
[48,"PPR闸阀","DN25","壁厚≥3.5mm/压力等级：S3.2/材质：聚丙烯/符合：GB/T18742.1-2017 GB/T18742.2-2017/颜色综合","个"]
[49,"PPR闸阀","DN32","壁厚≥3.5mm/压力等级：S3.2/材质：聚丙烯/符合：GB/T18742.1-2017 GB/T18742.2-2017/颜色综合","个"]
[50,"PPR闸阀","DN40","壁厚≥6mm/压力等级：S3.2/材质：聚丙烯/符合：GB/T18742.1-2017 GB/T18742.2-2017/颜色综合","个"]
[51,"PPR闸阀","DN50","壁厚≥6mm/压力等级：S3.2/材质：聚丙烯/符合：GB/T18742.1-2017 GB/T18742.2-2017/颜色综合","个"]
[52,"单冷高弯水龙头","综合","阀体材质：黄铜，表面镀铬，陶瓷阀芯/气泡出水、左右选择、冷热混水，冷热水标签/尺寸综合/配件:标配304不锈钢软管/符合国家标准。","个"]
[53,"冷热水高弯水龙头","综合","阀体材质：黄铜，表面镀铬，陶瓷阀芯/气泡出水、左右选择、冷热混水，冷热水标签/尺寸综合/配件:标配304不锈钢软管/符合国家标准。","个"]
[54,"洗手盆水龙头（单孔）","冷热水","阀体材质：黄铜，表面镀铬，陶瓷阀芯，净重≥1000g，符合国家标准","个"]
[55,"洗手盆水龙头（双孔）","冷热水","阀体材质：黄铜，表面镀铬，陶瓷阀芯，净重≥600g，符合国家标准","个"]
[56,"洗手盆水龙头","单冷","阀体材质：黄铜，表面镀铬，陶瓷阀芯，净重≥800g，符合国家标准","个"]
[57,"一进二出水咀","通用","快开把手，阀体材质：黄铜，表面镀铬，陶瓷阀芯，净重≥300g","个"]
[58,"水咀","通用","快开把手，阀体材质：黄铜，表面镀铬，陶瓷阀芯，净重≥150g","个"]
[59,"加长水咀","通用","长度16-20cm。快开把手，阀体材质：304不锈钢，黄铜阀芯","个"]
[60,"冷热水感应水龙头","综合","材质：黄铜主体/功能：感应出水、电池和插电供电可选，1秒出水，气泡出水，感应距离8-20cm/表面处理：PVD电镀/适用水压：最低≤0.05MPa，最高≥0.36MPa，出水量2L/分钟（正负10%）/尺寸及配件：尺寸综合，配交直流电控制盒（6v直流/220V交流）/含冷热调温阀","个"]
[61,"单冷感应水龙头","综合","材质：黄铜主体/表面处理：PVD电镀/功能：感应出水、电池和插电供电可选，1秒出水，气泡出水，感知距离250mm以内/适用水压：最低≤0.05MPa，最高≥0.36MPa，出水量2L/分钟（正负10%）/尺寸及配件：尺寸综合，配交直流电控制盒（6v直流/220V交流）","个"]
[62,"球阀1","DN20","活接、丝接综合，阀芯材质：黄铜阀体、铜阀芯，主体材质：铜。表面镀镍处理，手柄：不锈钢。公称压力≤1.6MPa","个"]
[63,"球阀2","DN25","活接、丝接综合，阀芯材质：黄铜阀体、铜阀芯，主体材质：铜。表面镀镍处理，手柄：不锈钢。公称压力≤1.6MPa","个"]
[64,"球阀3","DN32","活接、丝接综合，阀芯材质：黄铜阀体、铜阀芯，主体材质：铜。表面镀镍处理，手柄：不锈钢。公称压力≤1.6MPa","个"]
[65,"球阀4","DN50","活接、丝接综合，阀芯材质：黄铜阀体、铜阀芯，主体材质：铜。表面镀镍处理，手柄：不锈钢。公称压力≤1.6MPa","个"]
[66,"球阀5","DN63","活接、丝接综合，阀芯材质：黄铜阀体、铜阀芯，主体材质：铜。表面镀镍处理，手柄：不锈钢。公称压力≤1.6MPa","个"]
[67,"暗杆闸阀","DN40","PN16,球墨铸铁、法兰连接、软密封","个"]
[68,"暗杆闸阀","DN50","PN16,球墨铸铁、法兰连接、软密封","个"]
[69,"暗杆闸阀","DN65","PN16,球墨铸铁、法兰连接、软密封","个"]
[70,"暗杆闸阀","DN80","PN16,球墨铸铁、法兰连接、软密封","个"]
[71,"卧式止回阀","DN15","黄铜，挡板式，螺纹连接、活接综合","个"]
[72,"卧式止回阀","DN20","黄铜，挡板式，螺纹连接、活接综合","个"]
[73,"卧式止回阀","DN25","黄铜，挡板式，螺纹连接、活接综合","个"]
[74,"卧式止回阀","DN32","黄铜，挡板式，螺纹连接、活接综合","个"]
[75,"卧式止回阀","DN40","黄铜，挡板式，螺纹连接、活接综合","个"]
[76,"立式止回阀","DN15","黄铜，弹簧式，螺纹连接、活接综合","个"]
[77,"立式止回阀","DN20","黄铜，弹簧式，螺纹连接、活接综合","个"]
[78,"立式止回阀","DN25","黄铜，弹簧式，螺纹连接、活接综合","个"]
[79,"立式止回阀","DN32","黄铜，弹簧式，螺纹连接、活接综合","个"]
[80,"立式止回阀","DN40","黄铜，弹簧式，螺纹连接、活接综合","个"]
[81,"截止阀","DN20","全铜材质，螺纹连接、活接综合","个"]
[82,"截止阀","DN25","全铜材质，螺纹连接、活接综合","个"]
[83,"截止阀","DN32","全铜材质，螺纹连接、活接综合","个"]
[84,"截止阀","DN40","全铜材质，螺纹连接、活接综合","个"]
[85,"截止阀","DN50","全铜材质，螺纹连接、活接综合","个"]
[86,"截止阀7","DN63","全铜材质，螺纹连接、活接综合","个"]
[87,"不锈钢角阀","规格20#","冷热综合，304不锈钢主体,陶瓷阀芯","个"]
[88,"蹲便器延时脚踏阀","综合","黄铜阀体表面镀铬，黄铜阀芯，阀体净重≥600g","个"]
[89,"洗手盆普通型脚踏阀","综合","阀黄铜阀体表面镀铬，铜杆阀芯，普通阀体净重≥380g，","个"]
[90,"洗手盆斜式脚踏阀","综合","阀黄铜阀体表面镀铬，铜杆阀芯，普通阀体净重≥500g，","个"]
[91,"花洒混水阀","综合","黄铜主体，多层镀烙，陶瓷阀芯","个"]
[92,"电热水器混水阀","综合","黄铜主体，多层镀烙，陶瓷阀芯","个"]
[93,"水泵浮球阀","通用","符合国家标准","个"]
[94,"浮球阀","DN15","铜阀体（长度综合）、304不锈钢球体，304不锈钢杆","个"]
[95,"浮球阀","DN20","铜阀体（长度综合）、304不锈钢球体，304不锈钢杆","个"]
[96,"浮球阀","DN25","铜阀体（长度综合）、304不锈钢球体，304不锈钢杆","个"]
[97,"浮球阀","DN40","铜阀体（长度综合）、304不锈钢球体，304不锈钢杆","个"]
[98,"浮球阀","DN40双球","铜阀体（长度综合）、304不锈钢球体，304不锈钢杆","个"]
[99,"浮球阀","DN50","铜阀体（长度综合）、304不锈钢球体，304不锈钢杆","个"]
[100,"浮球阀","DN65","铜阀体（长度综合）、304不锈钢球体，304不锈钢杆","个"]
[101,"成套洁具类"]
[102,"交流一体式感应小便池","落地、挂墙综合综合","材质：陶瓷釉面材质/给水口径：DN15/适用水压:适用水压范围在大于等于范围0.05-0.6MPa/冲水量:0.5 升/次(正负10%）/感应距离大于等于范围25-100CM","个"]
[103,"直流一体式感应小便池","落地、挂墙综合综合","材质：陶瓷釉面材质/给水口径：DN15/适用水压:适用水压范围在大于等于范围0.05-0.6MPa/冲水量:0.5 升/次(正负10%）/感应距离大于等于范围25-100CM","个"]
[104,"挂式小便器","综合","材质：陶瓷釉面材质/给水口径：DN15/适用水压:适用水压范围在大于等于范围0.05-0.6MPa","个"]
[105,"立式小便器","综合","材质：陶瓷釉面材质/给水口径：DN15/适用水压:适用水压范围在大于等于范围0.05-0.6MPa","个"]
[106,"陶瓷洗手盆","立柱形","高温烧制洁釉面，符合国家标准，满足采购人需求。","个"]
[107,"淋浴器","软管1.5m长","含花洒、软管、底座，主体材质ABS塑料，电镀工艺","个"]
[108,"不带水箱蹲式大便器","尺寸综合","陶瓷防臭/存水弯综合/前后排水综合","个"]
[109,"带水箱蹲式大便器","尺寸综合","陶瓷防臭/存水弯综合/前后排水综合","个"]
[110,"坐式大便器","尺寸综合","主体材质:陶瓷/冲水原理:虹吸式/带水箱/水效等级1级/带水箱成品整套/","个"]
[111,"拖布池","尺寸综合","陶瓷/自带下水器","个"]
[112,"洗涤盆","尺寸综合","陶瓷/台上台下综合","个"]
[113,"SUS304不锈钢单盆","（40*50±5）cm","包含配件","个"]
[114,"塑料地漏","DN50","功能：具有防臭、防堵功能/尺寸及配件：圆形、方形综合，清扫口尺寸综合符合国家标准。","个"]
[115,"304不锈钢地漏","DN50","尺寸及配件：圆形、方形综合，清扫口尺寸综合/功能：具有防臭、防堵功能/符合国家标准。","个"]
[116,"蹲便器冲水水箱","综合","材质：箱体PP、核心水件ABS/功能：过滤防堵，双档按压，挂壁式安装/尺寸及配件：尺寸综合，排水量综合，含排水管等配件","个"]
[117,"淋浴喷头","通用","主材ABS塑料电镀，三档调节","个"]
[118,"配件"]
[119,"PVC地漏盖",110,"高度≥42mm，","个"]
[120,"PVC地漏盖",50,"高度≥28mm，","个"]
[121,"PVC地漏盖",75,"厚度≥34mm，","个"]
[122,"喷头座子","通用","材质：ABS塑料电镀","个"]
[123,"热水器铜三通","综合","材质：黄铜主体","个"]
[124,"软连接","100cm","外包编制不锈钢钢丝采用304#不锈钢钢丝 ，铜头子，内管TPV或PEX材质，承压≥3.5Mpa","根"]
[125,"软连接","80cm","外包编制不锈钢钢丝采用304#不锈钢钢丝 ，铜头子，内管TPV或PEX材质，承压≥3.5Mpa","根"]
[126,"软连接","60cm","外包编制不锈钢钢丝采用304#不锈钢钢丝 ，铜头子，内管TPV或PEX材质，承压≥3.5Mpa","根"]
[127,"软连接","50cm","外包编制不锈钢钢丝采用304#不锈钢钢丝 ，铜头子，内管TPV或PEX材质，承压≥3.5Mpa","根"]
[128,"软连接","40cm","外包编制不锈钢钢丝采用304#不锈钢钢丝 ，铜头子，内管TPV或PEX材质，承压≥3.5Mpa","根"]
[129,"软连接","30cm","外包编制不锈钢钢丝采用304#不锈钢钢丝 ，铜头子，内管TPV或PEX材质，承压≥3.5Mpa","根"]
[130,"防臭型下水伸缩管","综合","1.产品材质：ABS+PP管体，加厚/密封材质：硅橡胶","根"]
[131,"喷头连接管","通用","长：1.5m，黄铜头.不锈钢材质，内管PVC","根"]
[132,"洗手盆下水翻板","SQ-11","304不锈钢制","个"]
[133,"小便池明装感应开关","综合（成套）","电源：直流6V/进水口径DN15，出水口径DN15，水量可调，适合水压：0.5-0.8MPa/感应范围可调/阀体：黄铜，多层电镀工艺；不锈钢弯管","个"]
[134,"小便池暗装感应开关","综合（成套）","电源AC：200V-DC;6V/进水口径DN15，出水口径DN15/适合水压：0.5-0.8MPa","个"]
[135,"感应水龙头电磁阀","综合","长度可选，角度可选，DC/6伏/待机： ≤0.5mW","个"]
[136,"感应水龙头感应器","通用","通用型感应水龙头感应器，尺寸、规格型号综合","个"]
[137,"小便池漏斗","7.5-13cm","材质：塑料","个"]
[138,"小便池延时开关1","小体","黄铜阀体、电镀表面、黄铜阀芯、适用水压0.05MPA-0.8MPA","个"]
[139,"小便池延时开关2","中体","黄铜阀体、电镀表面、黄铜阀芯、适用水压0.05MPA-0.8MPA","个"]
[140,"小便池延时开关3","大体","黄铜阀体、电镀表面、黄铜阀芯、适用水压0.05MPA-0.8MPA","个"]
[141,"SUS304不锈钢尾冲管","32#","厚度≥1mm","根"]
[142,"座便按钮","规格综合","材质ABS","个"]
[143,"马桶盖塑料","通用","材质：PP塑料，盖体厚度不小于7.9mm","个"]
[144,"马桶进水阀","通用","适用水压0.1-16kg/cm²","个"]
[145,"马桶出水阀","通用","整套","个"]
[146,"马桶合页","无","材质：不锈钢","个"]
[147,"不锈钢耐震压力表1","Φ60","水压、气压、油压通用，铜弹簧、铜机芯、铜接头","个"]
[148,"不锈钢耐震压力表2","Φ100","水压、气压、油压通用，铜弹簧、铜机芯、铜接头","个"]
[149,"不锈钢耐震压力表3","Φ150","水压、气压、油压通用，铜弹簧、铜机芯、铜接头","个"]
[150,"不锈钢表弯","M14×1.5","304材质，角度综合","个"]
[151,"不锈钢表弯","M20×1.5","304材质，角度综合","个"]
[152,"无油生料带","综合","12mm宽*0.1mm厚/15米长","个"]
[153,"铸铁雨水斗","尺寸综合","DN150","个"]
[154,"铸铁雨水斗","尺寸综合","DN100","个"]
[155,"螺纹塑料堵头","Φ20-25","综合","个"]
[156,"螺纹塑料堵头","Φ30-35","综合","个"]
[157,"不锈钢螺纹堵头","Φ20","综合","个"]
[158,"不锈钢螺纹堵头","Φ25","综合","个"]
[159,"不锈钢螺纹堵头","Φ32","综合","个"]
[160,"PPR堵帽","Φ20-25","综合","个"]
[161,"PPR堵帽","Φ30-35","综合","个"]
[162,"2、电工类"]
[163,"成套灯具"]
[164,"LED灯管T8","9-10W ","LED日光灯，电压220V.色温综合，铜质电镀银针脚，长度综合","支"]
[165,"LED灯管T8","12-14W ","LED日光灯，电压220V.色温综合，铜质电镀银针脚，长度综合","支"]
[166,"LED灯管T8","18-20W","LED日光灯，电压220V.色温综合，铜质电镀银针脚，长度综合","支"]
[167,"LED灯管T8","18-20W","LED日光灯，电压220V.色温综合，铜质电镀银针脚，长度综合","支"]
[168,"LED灯管T5","9-10W ","LED日光灯，电压220V.色温综合，铜质电镀银针脚，长度综合","支"]
[169,"LED灯管T5","12-14W ","LED日光灯，电压220V.色温综合，铜质电镀银针脚，长度综合","支"]
[170,"LED灯管T5","18-20W","LED日光灯，电压220V.色温综合，铜质电镀银针脚，长度综合","支"]
[171,"LED灯管T5","18-20W","LED日光灯，电压220V.色温综合，铜质电镀银针脚，长度综合","支"]
[172,"单管T5/T8支架灯","不带罩","18-20w，LED日光灯，电压220V.烤漆铁艺支架","套"]
[173,"单管T5/T8支架灯","带罩","18-20w，LED日光灯，电压220V.烤漆铁艺支架","套"]
[174,"一体化LED长条灯","T5/14-16w","白光/暖白/暖黄三色、一体化可串联，电压220V，形状综合。","套"]
[175,"双管T5/T8支架灯","不带罩","2*18-20w，LED日光灯，电压220V.烤漆铁艺支架","套"]
[176,"双管T5/T8支架灯","带罩","2*18-20w，LED日光灯，电压220V.烤漆铁艺支架","套"]
[177,"三管T5/T8支架灯","3×16-18W 250V","3*18-20w，LED日光灯，电压220V.烤漆铁艺支架","套"]
[178,"单管T5/T8灯支架","不带罩","双边供电，电压220V，普通开关控制，烤漆铁艺支架","套"]
[179,"单管T5/T8灯支架灯","带罩","双边供电，电压220V，普通开关控制，烤漆铁艺支架","套"]
[180,"双管T5/T8灯支架灯","不带罩","双边供电，电压220V，普通开关控制，烤漆铁艺支架","套"]
[181,"双管T5/T8灯支架灯","带罩","双边供电，电压220V，普通开关控制，烤漆铁艺支架","套"]
[182,"防爆型双管灯-吊架","2*18-20w","Ex防爆标志,电压220V.压铸铝材灯体+钢化玻璃灯管+铁艺灯罩+钢网","套"]
[183,"防爆型单管灯-吊架","18-20w","Ex防爆标志,电压220V.压铸铝材灯体+钢化玻璃灯管+铁艺灯罩+钢网","套"]
[184,"单管防爆灯管T8","18-20w","钢化玻璃灯管","套"]
[185,"单管防爆灯支架","T8","Ex防爆标志,电压220V.铁艺灯罩+钢网","套"]
[186,"一体化LED长条防爆灯","T8/40-45w","安装方式可选（吸盘杆子，壁挂式，链条吊装，链条挂钩装，U型支架式）钢化玻璃+铁艺灯罩防护,防冲击钢网","套"]
[187,"LED灯带","8-10W/m","单色，100-120（颗/米），防尘等级IP2X，电压220V.色温（3300K-5000K）","m"]
[188,"LED灯泡","12-14W","电压220V.色温可选，尺寸综合","个"]
[189,"LED灯泡","18-20W","电压220V.色温可选，尺寸综合","个"]
[190,"LED灯泡","30-33W","电压220V.色温可选，尺寸综合","个"]
[191,"白炽灯灯泡","100-105W","电压：220V钨丝发热光源，E27螺口，暖黄光","个"]
[192,"白炽灯灯泡","50-55W螺口","电压：220V钨丝发热光源，E27螺口，暖黄光","个"]
[193,"球形灯泡彩色","22-25W","电压：220V,E27,三种色温可选：2700K.4000K.6500K","个"]
[194,"磨砂灯泡","22-25W","电压：220V，E27,磨砂灯泡红色","个"]
[195,"LED吸顶灯","18-20W","灯身材质：亚克力，电压220V.色温4000k或6500k，形状尺寸综合","个"]
[196,"LED吸顶灯","24-26W","灯身材质：亚克力，电压220V.色温4000k或6500k，形状尺寸综合","个"]
[197,"LED吸顶灯","36-38W","灯身材质：亚克力，电压220V.色温4000k或6500k，形状尺寸综合","个"]
[198,"LED吸顶灯","48-50W","灯身材质：亚克力，电压220V.色温4000k或6500k，形状尺寸综合","个"]
[199,"LED平板灯300mm*300mm","20-22W","安装形式综合，铝型材边框、铁壳背板、电压220V.色温4000k或6500k","个"]
[200,"LED平板灯300mm*600mm","36-38W","安装形式综合，铝型材边框、铁壳背板、电压220V.色温4000k或6500k","个"]
[201,"LED平板灯600mm*600mm","48-50W","安装形式综合，铝型材边框、铁壳背板、电压220V.色温4000k或6500k","个"]
[202,"LED平板灯1200mm*300mm","48-50W","安装形式综合，铝型材边框、铁壳背板、电压220V.色温4000k或6500k","个"]
[203,"LED投光灯","100-105W","\n防护等级IP65,灯身面罩:钢化玻璃,灯体一体化压铸铝，电压220V.色温6500K.","个"]
[204,"LED投光灯","150-155W","\n防护等级IP65,灯身面罩:钢化玻璃,灯体一体化压铸铝，电压220V.色温6500K","个"]
[205,"LED柱形灯","20-22W","柱形泡，三种色温可选：2700K.4000K.6500K","个"]
[206,"LED节能灯","28-30W","三种色温可选：2700K.4000K.6500K","个"]
[207,"LED筒灯1","3-5W","产品色温可选：3000K.4000K.6500k,开孔尺寸和材质：综合，铝材框架，pc面罩，不锈钢弹簧卡扣。颜色可选","个"]
[208,"LED筒灯2","6-8W","产品色温可选：3000K.4000K.6500k,开孔尺寸和材质：综合，铝材框架，pc面罩，不锈钢弹簧卡扣。颜色可选","个"]
[209,"LED筒灯3","9-12W","产品色温可选：3000K.4000K.6500k,开孔尺寸和材质：综合，铝材框架，pc面罩，不锈钢弹簧卡扣。颜色可选","个"]
[210,"LED筒灯4","12-15W","产品色温可选：3000K.4000K.6500k,开孔尺寸和材质：综合，铝材框架，pc面罩，不锈钢弹簧卡扣。颜色可选","个"]
[211,"LED筒灯5","16-18W","产品色温可选：3000K.4000K.6500k,开孔尺寸和材质：综合，铝材框架，pc面罩，不锈钢弹簧卡扣。颜色可选","个"]
[212,"LED筒灯6","18-20W","产品色温可选：3000K.4000K.6500k,开孔尺寸和材质：综合，铝材框架，pc面罩，不锈钢弹簧卡扣。颜色可选","个"]
[213,"防爆型LED筒灯","50-55w","压铸铝材+玻璃灯罩","个"]
[214,"声光控半圆球灯","24-26w","灯身材质：亚克力，电压220V.色温4000k或6500k，形状尺寸综合","个"]
[215,"人体感应半圆球灯","24-26w","产品色温可选：3000K.4000K.6500k,开孔尺寸和材质：综合，铝材框架，pc面罩","个"]
[216,"人体感应筒灯","5寸","产品色温可选：3000K.4000K.6500k,开孔尺寸和材质：综合，铝材框架，pc面罩","个"]
[217,"壁灯","10-11W","LED光源、220V，色温可选，形状可选","个"]
[218,"壁灯","12-14W","LED光源、220V，色温可选，形状可选","个"]
[219,"壁灯","16-18W","LED光源、220V，色温可选，形状可选","个"]
[220,"壁灯","18-20w","LED光源、220V，色温可选，形状可选","个"]
[221,"壁灯","24-26W","LED光源、220V，色温可选，形状可选","个"]
[222,"壁灯","36-38W","LED光源、220V，色温可选，形状可选","个"]
[223,"防爆灯（壁灯）","36-38W","LED光源、220V，色温可选，形状可选，玻璃灯罩，压铸铝底盘，陶瓷灯头，压铸铝灯架","个"]
[224,"LED射灯","6-7W","电压220v，尺寸综合，色温可选，灯身材质铝","个"]
[225,"LED射灯","8-9W","电压220v，尺寸综合，色温可选，灯身材质铝","个"]
[226,"LED绿光（射树灯）","30-35W","防水等级IP65，电压220V，按装方式综合","个"]
[227,"智能型航空障碍灯","20-22W","防水等级IP65，电压220V，按装方式综合","个"]
[228,"双头格栅灯","2×10-12w","电压220V，操控方式综合，灯身材质压铸铝，尺寸综合","个"]
[229,"双头格栅灯","2×16-18w","电压220V，操控方式综合，灯身材质压铸铝，尺寸综合","个"]
[230,"防爆型格栅灯","300*1200mm","2*20-22W,带防爆标志EX，钢丝防护网，电压220V","个"]
[231,"防爆型格栅灯","600*600mm","3*20-22W,带防爆标志EX，钢丝防护网，电压220V","个"]
[232,"防潮灯","1×25-27W","LED光源、220V，安装方式可选，防护等级IP67，尺寸综合。","个"]
[233,"防爆型防潮灯","1×25-27W","LED光源、220V，安装方式可选，防护等级IP67，尺寸综合。","个"]
[234,"镜前灯","8-10W","LED光源、220v 壁装","个"]
[235,"镜前灯","12-14w","LED光源、220v 壁装","个"]
[236,"地脚灯","1-3w","LED光源、220v，人体感应控制+光控，颜色可选，安装方式可选","个"]
[237,"环形灯","24-26W","综合","个"]
[238,"开关、插座、电表"]
[239,"单联单控暗开关","250V10A","暗装跷板式开关，86型,阻燃PC.符合符合GB16915.1最新标准。","个"]
[240,"单联双控暗开关","250V10A","暗装跷板式开关，86型,阻燃PC.符合符合GB16915.1最新标准。","个"]
[241,"双联单控暗开关","250V10A","暗装跷板式开关，86型,阻燃PC.符合符合GB16915.1最新标准。","个"]
[242,"双联双控暗开关","250V10A","暗装跷板式开关，86型,阻燃PC.符合符合GB16915.1最新标准。","个"]
[243,"三联单控暗开关","250V10A","暗装跷板式开关，86型,阻燃PC.符合符合GB16915.1最新标准。","个"]
[244,"三联双控暗开关","250V10A","暗装跷板式开关，86型,阻燃PC.符合符合GB16915.1最新标准。","个"]
[245,"四联单控暗开关","250V10A","暗装跷板式开关，86型,阻燃PC.符合符合GB16915.1最新标准。","个"]
[246,"四联双控暗开关","250V10A","暗装跷板式开关，86型,阻燃PC.符合符合GB16915.1最新标准。","个"]
[247,"单联单控明开关","250V10A","暗装跷板式开关，86型,阻燃PC.符合符合GB16915.1最新标准。","个"]
[248,"单联双控明开关","250V10A","暗装跷板式开关，86型,阻燃PC.符合符合GB16915.1最新标准。","个"]
[249,"双联单控明开关","250V10A","暗装跷板式开关，86型,阻燃PC.符合符合GB16915.1最新标准。","个"]
[250,"双联双控明开关","250V10A","暗装跷板式开关，86型,阻燃PC.符合符合GB16915.1最新标准。","个"]
[251,"三联单控明开关","250V10A","暗装跷板式开关，86型,阻燃PC.符合符合GB16915.1最新标准。","个"]
[252,"三联双控明开关","250V10A","暗装跷板式开关，86型,阻燃PC.符合符合GB16915.1最新标准。","个"]
[253,"明装三孔插座","16A","86型，阻燃PC.符合GB16915.1最新标准。","个"]
[254,"明装四孔插座","16A","86型，阻燃PC.符合GB16915.1最新标准。","个"]
[255,"明装五孔插座","10A","86型，阻燃PC.符合GB16915.1最新标准。","个"]
[256,"明装一开三孔插座","16A","86型，阻燃PC.符合GB16915.1最新标准。","个"]
[257,"明装一开五孔插座","10A","86型，阻燃PC.符合GB16915.1最新标准。","个"]
[258,"暗装三孔插座","16A","86型，阻燃PC.符合GB16915.1最新标准。","个"]
[259,"暗装四孔插座","10A","86型，阻燃PC.符合GB16915.1最新标准。","个"]
[260,"暗装五孔插座","10A","86型，阻燃PC.符合GB16915.1最新标准。","个"]
[261,"五孔地插","10A","表面不锈钢，内部阻燃PC.符合GB16915.1最新标准。","个"]
[262,"暗装一开三孔插座","16A","86型，阻燃PC.符合GB16915.1最新标准。","个"]
[263,"暗装一开五孔插座","10A","86型，阻燃PC.符合GB16915.1最新标准。","个"]
[264,"暗装漏电插座","16A","86型，阻燃PC.符合GB16915.1最新标准。","个"]
[265,"防爆防腐型一位单级开关","10A250V","EX防爆标识，铝合金压铸成型，防爆等级:ExdIBT6","个"]
[266,"防爆防腐型二位单级开关","10A250V","EX防爆标识，铝合金压铸成型，防爆等级:ExdIBT6","个"]
[267,"防爆防腐型三位单级开关","10A250V","EX防爆标识，铝合金压铸成型，防爆等级:ExdIBT6","个"]
[268,"防爆安全型三孔插座","16A","EX防爆标识，铝合金压铸成型，防爆等级:ExdIBT6，明装暗装综合","个"]
[269,"防爆安全型二孔连三孔插座","10A","EX防爆标识，铝合金压铸成型，防爆等级:ExdIBT6，明装暗装综合","个"]
[270,"底盒","明/暗装综合","86型阻燃PC","个"]
[271,"塑料接线盒","86型","阻燃PC","个"]
[272,"塑料接线盒","125型","阻燃PC","个"]
[273,"钢制接线盒","86型","钢制","个"]
[274,"钢制接线盒","125型","钢制","个"]
[275,"白面板","86型","86型阻燃PC","个"]
[276,"防触电插座保护盖","2相","1.86型防水盒","个"]
[277,"防触电插座保护盖","3相","1.86型防水盒","个"]
[278,"1位插线板","16A 1-1.2m线","带总控开关，带漏保，额定电压250V","个"]
[279,"2位插线板","10A 1.8-2.0m线","带总控开关，250V, 阻燃线，线芯1mm²","个"]
[280,"3位插线板","10A 1.8-2.0m线","带总控开关，250V, 阻燃线，线芯1mm²","个"]
[281,"4位插线板","10A 1.8-2m线","带总控开关，250V, 阻燃线，线芯1mm²","个"]
[282,"4位插线板","10A 3-3.2m线","带总控开关，250V, 阻燃线，线芯1mm²","个"]
[283,"6位插线板","10A 1.8-2m线","带总控开关，250V, 阻燃线，线芯1mm²","个"]
[284,"6位插线板","10A 3-3.2m线","带总控开关，250V, 阻燃线，线芯1mm²","个"]
[285,"8位插线板","10A 1.8-2m线","带总控开关，250V, 阻燃线，线芯1mm²","个"]
[286,"8位插线板","10A 3-3.2m线","带总控开关，250V, 阻燃线，线芯1mm²","个"]
[287,"2位插线板","10A 无线","带总控开关，250V, 阻燃线，线芯1mm²","个"]
[288,"4位插线板","10A 无线","带总控开关，250V, 阻燃线，线芯1mm²","个"]
[289,"6位插线板","10A 无线","带总控开关，250V, 阻燃线，线芯1mm²","个"]
[290,"三脚插头","16A","单相两极带接地可拆线插头","个"]
[291,"三脚插头","10A","单相两极带接地可拆线插头","个"]
[292,"二线插头","10A","单相两极带接地可拆线插头","个"]
[293,"单相电表","1.5（6A）","电压220V.总位数6位.小数位数1位，符合GB/T17215.321-2008标准。","个"]
[294,"单相电表","2.5（10A）","电压220V.总位数6位.小数位数1位，符合GB/T17215.321-2008。","个"]
[295,"单相电表","5（20A）","电压220V.总位数6位.小数位数1位，符合GB/T17215.321-2008标准。","个"]
[296,"单相电表","5（30A）","电压220V.总位数6位.小数位数1位，符合GB/T17215.321-2008。","个"]
[297,"单相电表","10(40)A","电压220V.总位数6位.小数位数1位，符合GB/T17215.321-2008。","个"]
[298,"单相电表","15(60)A","电压220V.总位数6位.小数位数1位，符合GB/T17215.321-2008标准。","个"]
[299,"动力（三相四线直插式）电表","3×1.5(6)A","电压220V.总位数6位.小数位数1位，符合GB/T17215.321-2008标准。","个"]
[300,"动力（三相四线直插式）电表","3×5（20A）","电压220V.总位数6位.小数位数1位，符合GB/T17215.321-2008标准。","个"]
[301,"动力（三相四线直插式）电表","3×10(40)A","电压380V.总位数6位.小数位数1位，符合符合GB/T17215.321-2008。","个"]
[302,"动力（三相四线互感式）电表","100/5","电压380V.总位数6位.小数位数1位，符合符合GB/T17215.321-2008。","个"]
[303,"动力（三相四线互感式）电表","150/5","电压380V.总位数6位.小数位数1位，符合符合GB/T17215.321-2008。","个"]
[304,"动力（三相四线互感式）电表","200/5","电压380V.总位数6位.小数位数1位，符合符合GB/T17215.321-2008。","个"]
[305,"动力（三相四线互感式）电表","300/5","电压380V.总位数6位.小数位数1位，符合符合GB/T17215.321-2008。","个"]
[306,"动力（三相四线互感式）电表","400/5","电压380V.总位数6位.小数位数1位，符合符合GB/T17215.321-2008。","个"]
[307,"三相四线电子式导轨电能表","1.5（6）A","电子式电量显示，1.5（6）A,4P  485通讯","个"]
[308,"三相四线轨道式电能表","5（100）A","电子式电量显示，5（100）A  485通讯","个"]
[309,"三相多功能数显表","AC  3×（5）A","数子化面板、LED显示，阻燃材质，可测功率、电流、电压，远程485通讯","个"]
[310,"漏电空开","10-16A 1P+N","额定电压230/400V,外壳等级IP20，漏电额定动作电流值30mA，动作时间≤0.1s，短路极限分断电流≥6000A.符合GB10963.1标准。","个"]
[311,"漏电空开","20-25A 1P+N","额定电压230/400V,外壳等级IP20，漏电额定动作电流值30mA，动作时间≤0.1s，短路极限分断电流≥6000A.符合GB10963.1标准。","个"]
[312,"漏电空开","32-40A 1P+N","额定电压230/400V,外壳等级IP20，漏电额定动作电流值30mA，动作时间≤0.1s，短路极限分断电流≥6000A.符合GB10963.1标准。","个"]
[313,"漏电空开","63A 1P+N","额定电压230/400V,外壳等级IP20，漏电额定动作电流值30mA，动作时间≤0.1s，短路极限分断电流≥6000A.符合GB10963.1标准。","个"]
[314,"漏电空开","10-16A  2P","额定电压230/400V,外壳等级IP20，漏电额定动作电流值30mA，动作时间≤0.1s，短路极限分断电流≥6000A.符合GB10963.1标准。","个"]
[315,"漏电空开","20-25A  2P","额定电压230/400V,外壳等级IP20，漏电额定动作电流值30mA，动作时间≤0.1s，短路极限分断电流≥6000A.符合GB10963.1标准。","个"]
[316,"漏电空开","32A 2P","额定电压230/400V,外壳等级IP20，漏电额定动作电流值30mA，动作时间≤0.1s，短路极限分断电流≥6000A.符合GB10963.1标准。","个"]
[317,"漏电空开","63A 2P","额定电压230/400V,外壳等级IP20，漏电额定动作电流值30mA，动作时间≤0.1s，短路极限分断电流≥6000A.符合GB10963.1标准。","个"]
[318,"漏电空开","100A 3P","额定电压400V,外壳等级IP20，漏电额定动作电流值30mA，动作时间≤0.1s，短路极限分断电流≥6000A.符合GB10963.1标准。","个"]
[319,"漏电空开","16A 3P+N","额定电压400V,外壳等级IP20，漏电额定动作电流值30mA，动作时间≤0.1s，短路极限分断电流≥6000A.符合GB10963.1标准。","个"]
[320,"漏电空开","32A 3P+N","额定电压400V,外壳等级IP20，漏电额定动作电流值30mA，动作时间≤0.1s，短路极限分断电流≥6000A.符合GB10963.1。","个"]
[321,"漏电空开","63A 3P+N","额定电压400V,外壳等级IP20，漏电额定动作电流值30mA，动作时间≤0.1s，短路极限分断电流≥6000A符合GB10963.1标准。","个"]
[322,"漏电空开","100A 3P+N","额定电压400V,外壳等级IP20，漏电额定动作电流值30mA，动作时间≤0.1s，短路极限分断电流≥6000A.符合GB10963.1标准。","个"]
[323,"墙壁面板漏电保护开关","32A","带开关键、测试键，额定电压230VAC，动作时间<0.1s","个"]
[324,"空开","10A 1P","额定电压230/400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[325,"空开","16A 1P","额定电压230/400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[326,"空开","20A 1P","额定电压230/400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[327,"空开","25A 1P","额定电压230/400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[328,"空开","32A 1P","额定电压230/400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[329,"空开","40A 1P","额定电压230/400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[330,"空开","63A 1P","额定电压230/400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[331,"空开","10A 2P","额定电压400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[332,"空开","16A 2P","额定电压400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[333,"空开","20A 2P","额定电压400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[334,"空开","25A 2P","额定电压400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[335,"空开","32A 2P","额定电压400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[336,"空开","40A 2P","额定电压400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[337,"空开","63A 2P","额定电压400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[338,"空开","25A 3P","额定电压400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[339,"空开","32A 3P","额定电压400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[340,"空开","40A 3P","额定电压400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[341,"空开","63A 3P","额定电压400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[342,"空开","25A 4P","额定电压400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[343,"空开","63A 4P","额定电压400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[344,"空开","80A 4P","额定电压400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[345,"塑壳断式路器","3P 25A","额定电流：63A/飞弧距离≤50mm，分段能力/电压：25KA/400V，符合GB/T 14048.2最新标准。","个"]
[346,"塑壳断式路器","3P 32A","额定电流：63A/飞弧距离≤50mm，分段能力/电压：25KA/400V，符合GB/T 14048.2最新标准。。","个"]
[347,"塑壳断式路器","3P 63A","额定电流：63A/飞弧距离≤50mm，分段能力/电压：25KA/400V，符合GB/T 14048.2最新标准。","个"]
[348,"塑壳断式路器","3P 125A","额定电流：125A/飞弧距离≤50mm，分段能力/电压：25KA/400V，符合GB/T 14048.2最新标准。","个"]
[349,"塑壳断式路器","3P 250A","额定电流：250A/飞弧距离≤50mm，分段能力/电压：25KA/400V，符合GB/T 14048.2最新标准。","个"]
[350,"塑壳断式路器（漏电保护）","4P 250A","漏电电流可调，符合GB/T 14048.2最新标准。","个"]
[351,"塑壳断式路器（漏电保护）","4P 200A","漏电电流可调，符合GB/T 14048.2最新标准。","个"]
[352,"塑壳断式路器（漏电保护）","4P 160A","漏电电流可调，符合GB/T 14048.2最新标准。","个"]
[353,"塑壳断式路器（漏电保护）","4P 125A","漏电电流可调，符合GB/T 14048.2最新标准。","个"]
[354,"塑壳断式路器","3P 400A","额定电流：250A/飞弧距离≤50mm，分段能力/电压：25KA/400V，符合GB/T 14048.2最新标准。","个"]
[355,"隔离开关","32A 3P","额定电压400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[356,"隔离开关","63A 3P","额定电压400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[357,"隔离开关","100A 3P","额定电压400V,外壳等级IP20，短路极限分断电流≥6000A.符合GB10963.1最新标准。","个"]
[358,"一体式浪涌保护器IST 4P65KA","65KA  4P","防护等级IP40（前面板），IP20（端子），工作温度-25℃至 60℃，存储温度-40℃至 70℃符合标准：IEC 61643-11 和 EN 61643-11最新标准。","组"]
[359,"交流接触器","9A 220V","符合标准GB/T14048.4最新标准","个"]
[360,"交流接触器","12A 220V","符合标准GB/T14048.4最新标准","个"]
[361,"交流接触器","32A 220V","符合标准GB/T14048.4最新标准","个"]
[362,"交流接触器","9A 380V","符合标准GB/T14048.4最新标准","个"]
[363,"交流接触器","12A 380V","符合标准GB/T14048.4最新标准","个"]
[364,"交流接触器","32 380V","符合标准GB/T14048.4最新标准","个"]
[365,"时间控制器","AC220V","导轨式，整机功耗小于1w","个"]
[366,"时间控制器","AC380V","导轨式，整机功耗小于1w","个"]
[367,"时间控制器带插孔","10A","数显，250V","个"]
[368,"8脚5A中间继电器","DC12V 带底座","2开2闭,拔插式,带LED指示灯","个"]
[369,"8脚5A中间继电器","DC12V 不带底座","2开2闭,拔插式,带LED指示灯","个"]
[370,"8脚5A中间继电器","DC12V 带底座","2开2闭,拔插式,带LED指示灯,带测试按钮","个"]
[371,"8脚5A中间继电器","DC24V 带底座","2开2闭,拔插式,带LED指示灯","个"]
[372,"8脚5A中间继电器","DC24V 不带底座","2开2闭,拔插式,带LED指示灯","个"]
[373,"8脚5A中间继电器","DC24V 带底座","2开2闭,拔插式,带LED指示灯,带测试按钮","个"]
[374,"8脚5A中间继电器","AC12V 带底座","2开2闭,拔插式,带LED指示灯","个"]
[375,"8脚5A中间继电器","AC12V 不带底座","2开2闭,拔插式,带LED指示灯","个"]
[376,"8脚5A中间继电器","AC12V 带底座","2开2闭,拔插式,带LED指示灯,带测试按钮","个"]
[377,"8脚5A中间继电器","AC24V 带底座","2开2闭,拔插式,带LED指示灯","个"]
[378,"8脚5A中间继电器","AC24V 不带底座","2开2闭,拔插式,带LED指示灯","个"]
[379,"8脚5A中间继电器","AC24V 带底座","2开2闭,拔插式,带LED指示灯,带测试按钮","个"]
[380,"8脚5A中间继电器","AC230V 带底座","2开2闭,拔插式,带LED指示灯","个"]
[381,"8脚5A中间继电器","AC230V 不带底座","2开2闭,拔插式,带LED指示灯","个"]
[382,"8脚5A中间继电器","AC230V 带底座","2开2闭,拔插式,带LED指示灯,带测试按钮","个"]
[383,"8脚12A中间继电器","DC12V 带底座","2开2闭,拔插式,带LED指示灯","个"]
[384,"8脚12A中间继电器","DC12V 不带底座","2开2闭,拔插式,带LED指示灯","个"]
[385,"8脚12A中间继电器","DC12V 带底座","2开2闭,拔插式,带LED指示灯,带测试按钮","个"]
[386,"8脚12A中间继电器","DC24V 带底座","2开2闭,拔插式,带LED指示灯","个"]
[387,"8脚12A中间继电器","DC24V 不带底座","2开2闭,拔插式,带LED指示灯","个"]
[388,"8脚12A中间继电器","DC24V 带底座","2开2闭,拔插式,带LED指示灯,带测试按钮","个"]
[389,"8脚12A中间继电器","AC24V 带底座","2开2闭,拔插式,带LED指示灯","个"]
[390,"8脚12A中间继电器","AC24V 不带底座","2开2闭,拔插式,带LED指示灯","个"]
[391,"8脚12A中间继电器","AC24V 带底座","2开2闭,拔插式,带LED指示灯,带测试按钮","个"]
[392,"8脚12A中间继电器","AC230V 带底座","2开2闭,拔插式,带LED指示灯","个"]
[393,"8脚12A中间继电器","AC230V 不带底座","2开2闭,拔插式,带LED指示灯","个"]
[394,"8脚12A中间继电器","AC230V 带底座","2开2闭,拔插式,带LED指示灯,带测试按钮","个"]
[395,"14脚6A中间继电器","DC12V 带底座","2开2闭,拔插式,带LED指示灯","个"]
[396,"14脚6A中间继电器","DC12V 不带底座","2开2闭,拔插式,带LED指示灯","个"]
[397,"14脚6A中间继电器","DC12V 带底座","2开2闭,拔插式,带LED指示灯,带测试按钮","个"]
[398,"14脚6A中间继电器","DC24V 带底座","2开2闭,拔插式,带LED指示灯","个"]
[399,"14脚6A中间继电器","DC24V 不带底座","2开2闭,拔插式,带LED指示灯","个"]
[400,"14脚6A中间继电器","DC24V 带底座","2开2闭,拔插式,带LED指示灯,带测试按钮","个"]
[401,"14脚6A中间继电器","AC24V 带底座","2开2闭,拔插式,带LED指示灯","个"]
[402,"14脚6A中间继电器","AC24V 不带底座","2开2闭,拔插式,带LED指示灯","个"]
[403,"14脚6A中间继电器","AC24V 带底座","2开2闭,拔插式,带LED指示灯,带测试按钮","个"]
[404,"14脚6A中间继电器","AC230V 带底座","2开2闭,拔插式,带LED指示灯","个"]
[405,"14脚6A中间继电器","AC230V 不带底座","2开2闭,拔插式,带LED指示灯","个"]
[406,"14脚6A中间继电器","AC230V 带底座","2开2闭,拔插式,带LED指示灯,带测试按钮","个"]
[407,"电力管、线、槽、箱"]
[408,"护套线","BVVB 2*1.5mm²","符合JB/T8734.2最新标准，生产日期6个月以内","米"]
[409,"护套线","BVVB 2*2.5mm²","符合JB/T8734.2最新标准，生产日期6个月以内","米"]
[410,"护套线","BVVB 2*4mm²","符合JB/T8734.2最新标准，生产日期6个月以内","米"]
[411,"护套线","BVVB 2*6mm²","符合JB/T8734.2最新标准，生产日期6个月以内","米"]
[412,"护套线","BVVB 3*1.5mm²","符合JB/T8734.2最新标准，生产日期6个月以内","米"]
[413,"护套线","BVVB 3*2.5mm²","符合JB/T8734.2最新标准，生产日期6个月以内","米"]
[414,"护套线","BVVB 3*4mm²","符合JB/T8734.2最新标准，生产日期6个月以内","米"]
[415,"阻燃铜芯线","ZR-BV-1.5mm2","颜色综合，符合GB/T5023.3，GB/T 19666最新标准，生产日期6个月以内","米"]
[416,"阻燃铜芯线","ZR-BV-2.5mm2","颜色综合，符合GB/T5023.3，GB/T 19666最新标准，生产日期6个月以内","米"]
[417,"阻燃铜芯线","ZR-BV-4mm2","颜色综合，符合GB/T5023.3，GB/T 19666最新标准，生产日期6个月以内","米"]
[418,"阻燃铜芯线","ZR-BV-6mm2","颜色综合，符合GB/T5023.3，GB/T 19666最新标准，生产日期6个月以内","米"]
[419,"阻燃铜芯线","ZR-BV-10mm2","颜色综合，符合GB/T5023.3，GB/T 19666最新标准，生产日期6个月以内","米"]
[420,"电力电缆","YJV-0.6/1kV-2*2.5mm2","符合GB/T 12706.1最新标准","米"]
[421,"电力电缆","YJV-0.6/1kV-3*6mm2","符合GB/T 12706.1最新标准","米"]
[422,"电力电缆","YJV-0.6/1kV-4*6mm2","符合GB/T 12706.1最新标准","米"]
[423,"电力电缆","YJV-0.6/1kV-5*10 mm2","符合GB/T 12706.1最新标准","米"]
[424,"电力电缆","WDZB-YJY 5×4mm2","符合GB/T 12706.1,GB/T 19666最新标准","米"]
[425,"电力电缆","WDZB-YJY 5×6mm2","符合GB/T 12706.1,GB/T 19666最新标准","米"]
[426,"电力电缆","WDZB-YJY 5×10mm2","符合GB/T 12706.1,GB/T 19666最新标准","米"]
[427,"电力电缆","WDZB-YJY 5×16mm2","符合GB/T 12706.1,GB/T 19666最新标准","米"]
[428,"电力电缆","WDZB-YJY 4×25+1×16mm2","符合GB/T 12706.1,GB/T 19666最新标准","米"]
[429,"电力电缆","WDZB-YJY 4×35+1×16mm2","符合GB/T 12706.1,GB/T 19666最新标准","米"]
[430,"铠装电力电缆","WDZB-YJY 4×35+1×16mm2","符合GB/T 12706.1,GB/T 19666最新标准","米"]
[431,"电力电缆","WDZB-YJY 4×50+1×25mm2","符合GB/T 12706.1,GB/T 19666最新标准","米"]
[432,"铠装电力电缆","WDZB-YJY 4×50+1×25mm2","符合GB/T 12706.1,GB/T 19666最新标准","米"]
[433,"电力电缆","WDZB-YJY 4×70+1×35mm2","符合GB/T 12706.1,GB/T 19666最新标准","米"]
[434,"铠装电力电缆","WDZB-YJY 4×70+1×35mm2","符合GB/T 12706.1,GB/T 19666最新标准","米"]
[435,"电力电缆","WDZB-YJY 4×95+1×50mm2","符合GB/T 12706.1,GB/T 19666最新标准","米"]
[436,"铠装电力电缆","WDZB-YJY 4×95+1×50mm2","符合GB/T 12706.1,GB/T 19666最新标准","米"]
[437,"电力电缆","WDZB-YJY 4×120+1×70mm2","符合GB/T 12706.1,GB/T 19666最新标准","米"]
[438,"铠装电力电缆","WDZB-YJY 4×120+1×70mm2","符合GB/T 12706.1,GB/T 19666最新标准","米"]
[439,"电力电缆","WDZB-YJY 4×150+1×70mm2","符合GB/T 12706.1,GB/T 19666最新标准","米"]
[440,"铠装电力电缆","WDZB-YJY 4×150+1×70mm2","符合GB/T 12706.1,GB/T 19666最新标准","米"]
[441,"电力电缆","WDZB-YJY 4×185+1×95mm2","符合GB/T 12706.1,GB/T 19666最新标准","米"]
[442,"铠装电力电缆","WDZB-YJY 4×185+1×95mm2","符合GB/T 12706.1,GB/T 19666最新标准","米"]
[443,"电力电缆","WDZB-YJY 4×240+1×120mm2","符合GB/T 12706.1,GB/T 19666最新标准","米"]
[444,"铠装电力电缆","WDZB-YJY 4×240+1×120mm2","符合GB/T 12706.1,GB/T 19666最新标准","米"]
[445,"矿物绝缘电缆","BTTZ-5×10","符合GB/T 13033最新标准","米"]
[446,"矿物绝缘电缆","BTTZ-5×16","符合GB/T 13033最新标准","米"]
[447,"矿物绝缘电缆","BTTZ 4×25+1×16","符合GB/T 13033最新标准","米"]
[448,"矿物绝缘电缆","BTTZ-4×35+1×16","符合GB/T 13033最新标准","米"]
[449,"RVV铜芯橡套线","3×1.5M² ","颜色综合，符合GB/T5023.5或JB/T 8734.3最新标准，生产日期6个月以内","米"]
[450,"RVV铜芯橡套线","3×2.5M² ","颜色综合，符合GB/T5023.5或JB/T 8734.3最新标准，生产日期6个月以内","米"]
[451,"RVV铜芯橡套线","3×4M² ","颜色综合，符合GB/T5023.5或JB/T 8734.3最新标准，生产日期6个月以内","米"]
[452,"RVV铜芯橡套线","3×6M² ","颜色综合，符合GB/T5023.5或JB/T 8734.3最新标准，生产日期6个月以内","米"]
[453,"ZC-RVV铜芯护套线","3×1.5M² ","颜色综合，符合GB/T5023.5,GB/T 19666最新标准，生产日期6个月以内","米"]
[454,"ZC-RVV铜芯护套线","3×2.5M² ","颜色综合，符合GB/T5023.5,GB/T 19666最新标准，生产日期6个月以内","米"]
[455,"ZC-RVV铜芯护套线","3×4M² ","颜色综合，符合GB/T5023.5,GB/T 19666最新标准，生产日期6个月以内","米"]
[456,"ZC-RVV铜芯护套线","3×6M² ","颜色综合，符合GB/T5023.5,GB/T 19666最新标准，生产日期6个月以内","米"]
[457,"电话线","2*0.5mm²","无氧铜芯，柔韧PVC外被","米"]
[458,"电视闭路线                  ","1mm²","1mm²铜芯，环保新料，铝镁编织屏蔽层,阻燃屏蔽。","米"]
[459,"闭路线插头","B5","适用于各种电视","个"]
[460,"电话连接线","1.5mm","阻燃PC","根"]
[461,"电缆桥架","100×100×1.0mm（宽*高*厚）mm","镀锌","米"]
[462,"桥架连接件","适配100×100桥架","镀锌","个"]
[463,"电缆桥架","200×100×1.0mm（宽*高*厚）mm","镀锌","米"]
[464,"桥架连接件","适配200×100桥架","镀锌","个"]
[465,"电缆桥架","300×100×1.0（宽*高*厚）mm","镀锌","米"]
[466,"桥架连接件","适配300×100桥架","镀锌","个"]
[467,"电缆桥架","400×100×1.2（宽*高*厚）mm","镀锌","米"]
[468,"桥架连接件","适配400×100桥架","镀锌","个"]
[469,"电缆桥架","500×100×1.2（宽*高*厚）mm","镀锌","米"]
[470,"桥架连接件","适配500×100桥架","镀锌","个"]
[471,"电缆桥架","600×100×1.5（宽*高*厚）mm","镀锌","米"]
[472,"桥架连接件","适配600×100桥架","镀锌","个"]
[473,"电缆桥架","800×100×2（宽*高*厚）mm","镀锌","米"]
[474,"桥架连接件","适配800×100桥架","镀锌","个"]
[475,"电缆桥架","500×150×1.5（宽*高*厚）mm","镀锌","米"]
[476,"桥架连接件","适配500×150桥架","镀锌","个"]
[477,"电缆桥架","600×150×1.5（宽*高*厚）mm","镀锌","米"]
[478,"桥架连接件","适配600×150桥架","镀锌","个"]
[479,"阻燃绝缘PVC-U槽板","20*10mm","符合QB/T1614最新标准","米"]
[480,"阻燃绝缘PVC-U槽板连接件","适配20*10mm槽板 ","符合QB/T1614最新标准","个"]
[481,"阻燃绝缘PVC-U槽板","24*14mm","符合QB/T1614最新标准","米"]
[482,"阻燃绝缘PVC-U槽板连接件","适配24*14mm槽板 ","符合QB/T1614最新标准","个"]
[483,"阻燃绝缘PVC-U槽板","30*15mm","符合QB/T1614最新标准","米"]
[484,"阻燃绝缘PVC-U槽板连接件","适配30*15mm槽板 ","符合QB/T1614最新标准","个"]
[485,"阻燃绝缘PVC-U槽板","39*19mm","符合QB/T1614最新标准","米"]
[486,"阻燃绝缘PVC-U槽板连接件","适配39*19mm槽板 ","符合QB/T1614最新标准","个"]
[487,"阻燃绝缘PVC-U槽板","50*25mm","符合QB/T1614最新标准","米"]
[488,"阻燃绝缘PVC-U槽板连接件","适配50*25mm槽板 ","符合QB/T1614最新标准","个"]
[489,"阻燃绝缘PVC-U槽板","60*40mm","符合QB/T1614最新标准","米"]
[490,"阻燃绝缘PVC-U槽板连接件","适配60*40mm槽板 ","符合QB/T1614最新标准","个"]
[491,"阻燃绝缘PVC-U槽板","80*40mm","符合QB/T1614最新标准","米"]
[492,"阻燃绝缘PVC-U槽板连接件","适配80*40mm槽板 ","符合QB/T1614最新标准","个"]
[493,"阻燃绝缘PVC-U槽板","100*40mm","符合QB/T1614最新标准","米"]
[494,"阻燃绝缘PVC-U槽板连接件","适配100*40mm槽板 ","符合QB/T1614最新标准","个"]
[495,"阻燃绝缘PVC-U槽板","100*50mm","符合QB/T1614最新标准","米"]
[496,"阻燃绝缘PVC-U槽板连接件","适配100*50mm槽板 ","符合QB/T1614最新标准","个"]
[497,"pvc弧形地槽板","100mm","厚度不小于2mm，阻燃绝缘，","米"]
[498,"pvc弧形地槽板连接件","适配100mm地槽板","厚度不小于2mm，阻燃绝缘，","个"]
[499,"pvc弧形地槽板","75mm","厚度不小于2mm，阻燃绝缘，","米"]
[500,"pvc弧形地槽板连接件","适配75mm地槽板","厚度不小于2mm，阻燃绝缘，","个"]
[501,"pvc弧形地槽板","60mm","厚度不小于2mm，阻燃绝缘，","米"]
[502,"pvc弧形地槽板连接件","适配60mm地槽板","厚度不小于2mm，阻燃绝缘，","个"]
[503,"pvc弧形地槽板","50mm","厚度不小于2mm，阻燃绝缘，","米"]
[504,"pvc弧形地槽板连接件","适配50mm地槽板","厚度不小于2mm，阻燃绝缘，","个"]
[505,"铝合金弧形地槽板","宽30-32mm","自带背胶，颜色综合","米"]
[506,"铝合金弧形地槽板","宽40-42mm","自带背胶，颜色综合","米"]
[507,"铝合金弧形地槽板","宽48-50mm","自带背胶，颜色综合","米"]
[508,"铝合金弧形地槽板","宽56-58mm","自带背胶，颜色综合","米"]
[509,"防水型可绕金属套管","公称口径15","阻燃，外层微柔韧性聚氯乙烯(PVC)包覆","米"]
[510,"防水型可绕金属套管","公称口径17","阻燃，外层微柔韧性聚氯乙烯(PVC)包覆","米"]
[511,"防水型可绕金属套管","公称口径24","阻燃，外层微柔韧性聚氯乙烯(PVC)包覆","米"]
[512,"防水型可绕金属套管","公称口径30","阻燃，外层微柔韧性聚氯乙烯(PVC)包覆","米"]
[513,"PVC硬质线穿管","DN16mm","壁厚1.4-1.5mm，含管件,符合JG 3050最新标准","米"]
[514,"PVC硬质线穿管","DN20mm","壁厚1.6-1.8mm，含管件,符合JG 3050最新标准","米"]
[515,"PVC硬质线穿管","DN25mm","壁厚1.8-2.0mm，含管件,符合JG 3050最新标准","米"]
[516,"PVC硬质线穿管","DN32mm","壁厚2.0-2.2mm，含管件,符合JG 3050最新标准","米"]
[517,"黄腊管","Ø8mm","聚缘阻燃","米"]
[518,"黄腊管","Ø10mm","聚缘阻燃","米"]
[519,"黄腊管","Ø12mm","聚缘阻燃","米"]
[520,"黄腊管","Ø14mm","聚缘阻燃","米"]
[521,"黄腊管","Ø16mm","聚缘阻燃","米"]
[522,"黄腊管","Ø20mm","聚缘阻燃","米"]
[523,"黄腊管","Ø25mm","聚缘阻燃","米"]
[524,"黄腊管","Ø30mm","聚缘阻燃","米"]
[525,"黄腊管","Ø35mm","聚缘阻燃","米"]
[526,"黄腊管","Ø40mm","聚缘阻燃","米"]
[527,"阻燃绝缘PVC电工波纹套管","公称外径16mm","符合JG3050最新标准。","米"]
[528,"阻燃绝缘PVC电工波纹套管","公称外径20mm","符合JG3050最新标准。","米"]
[529,"阻燃绝缘PVC电工波纹套管","公称外径25mm","符合JG3050最新标准。","米"]
[530,"阻燃绝缘PVC电工波纹套管","公称外径32mm","符合JG3050最新标准。","米"]
[531,"阻燃绝缘PVC电工波纹套管","公称外径40mm","符合JG3050最新标准。","米"]
[532,"阻燃绝缘PVC电工波纹套管","公称外径50mm","符合JG3050最新标准。","米"]
[533,"KBG/JDG穿线管",20,"厚度≥0.8mm，镀锌","米"]
[534,"KBG/JDG穿线管连接件","适配20穿线管","适配20穿线管","个"]
[535,"KBG/JDG穿线管",25,"厚度≥1mm，镀锌","米"]
[536,"KBG/JDG穿线管连接件","适配25穿线管","适配25穿线管","个"]
[537,"KBG/JDG穿线管",32,"厚度≥1mm，镀锌","米"]
[538,"KBG/JDG穿线管连接件","适配32穿线管","适配32穿线管","个"]
[539,"KBG/JDG穿线管",40,"厚度≥1.2mm，镀锌","米"]
[540,"KBG/JDG穿线管连接件","适配40穿线管","适配40穿线管","个"]
[541,"KBG/JDG穿线管",50,"厚度≥1.5mm，镀锌","米"]
[542,"KBG/JDG穿线管连接件","适配50穿线管","适配50穿线管","个"]
[543,"多媒体信息箱","300x400x100mm","优质冷轧钢板表面静电喷漆防锈处理","个"]
[544,"塑壳式空开箱","4位","全塑料明装/暗装综合，铁导轨；符合GB/T17466.1和GB/T17466.24最新标准。","个"]
[545,"塑壳式空开箱","6位","全塑料明装/暗装综合，铁导轨；符合GB/T17466.1和GB/T17466.24最新标准。","个"]
[546,"塑壳式空开箱","8位","全塑料明装/暗装综合，铁导轨；符合GB/T17466.1和GB/T17466.24最新标准。","个"]
[547,"塑壳式空开箱","9位","全塑料明装/暗装综合，铁导轨；符合GB/T17466.1和GB/T17466.24最新标准。","个"]
[548,"塑壳式空开箱","12位","全塑料明装/暗装综合，铁导轨；符合GB/T17466.1和GB/T17466.24最新标准。","个"]
[549,"钢制空开箱","4位","符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[550,"钢制空开箱","6位","符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[551,"钢制空开箱","8位","符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[552,"钢制空开箱","9位","符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[553,"钢制空开箱","12位","符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[554,"钢制空开箱","铁8位","符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[555,"室内钢制配电箱","250*200*140mm","厚度≥1mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[556,"室内钢制配电箱","300*250*140mm","厚度≥1mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[557,"室内钢制配电箱","400*300*140mm","厚度≥1mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[558,"室内钢制配电箱","400*300*200mm","厚度≥1mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[559,"室内钢制配电箱","400*300*250mm","厚度≥1mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[560,"室内钢制配电箱","500*400*140mm","厚度≥1mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[561,"室内钢制配电箱","500*400*200mm","厚度≥1mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[562,"室内钢制配电箱","600*400*200mm","厚度≥1.2mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[563,"室内钢制配电箱","600*500*200mm","厚度≥1.2mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[564,"室内钢制配电箱","600*500*250mm","厚度≥1.2mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[565,"室内钢制配电箱","700*500*200mm","厚度≥1.2mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[566,"室内钢制配电箱","700*500*250mm","厚度≥1.2mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[567,"室内钢制配电箱","800*600*250mm","厚度大于1.5mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[568,"室内钢制配电箱","800*600*250mm","厚度大于1.5mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[569,"室内钢制配电箱","1000*800*200mm","厚度大于1.5mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[570,"室内钢制配电箱","1000*800*250mm","厚度大于1.5mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[571,"室外钢制配电箱","600*400*200mm","厚度≥1.2mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[572,"室外钢制配电箱","600*500*200mm","厚度≥1.2mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[573,"室外钢制配电箱","600*500*250mm","厚度≥1.2mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[574,"室外钢制配电箱","700*500*200mm","厚度≥1.2mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[575,"室外钢制配电箱","700*500*250mm","厚度≥1.2mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[576,"室外钢制配电箱","800*600*250mm","厚度≥1.5mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[577,"室外钢制配电箱","800*600*250mm","厚度≥1.5mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[578,"室外钢制配电箱","1000*800*200mm","厚度≥1.5mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[579,"室外钢制配电箱","1000*800*250mm","厚度≥1.5mm，IP43,符合GB/T17466.1和GB/T17466.24最新标准。明装、暗装综合","个"]
[580,"室外304不锈钢配电箱","300*250*160mm","最薄处厚度≥0.6mm，挂墙、落地综合","个"]
[581,"室外304不锈钢配电箱","400*300*160mm","最薄处厚度≥0.6mm，挂墙、落地综合","个"]
[582,"室外304不锈钢配电箱","400*300*180mm","最薄处厚度≥0.6mm，挂墙、落地综合","个"]
[583,"室外304不锈钢配电箱","500*400*180mm","最薄处厚度≥0.8mm，挂墙、落地综合","个"]
[584,"室外304不锈钢配电箱","500*400*200mm","最薄处厚度≥0.8mm，挂墙、落地综合","个"]
[585,"室外304不锈钢配电箱","600*500*180mm","最薄处厚度≥0.8mm，挂墙、落地综合","个"]
[586,"室外304不锈钢配电箱","600*500*200mm","最薄处厚度≥0.8mm，挂墙、落地综合","个"]
[587,"室外304不锈钢配电箱","800*600*200mm","最薄处厚度≥0.8mm，挂墙、落地综合","个"]
[588,"室外304不锈钢配电箱","1000*600*350mm","最薄处厚度≥1.0mm，挂墙、落地综合","个"]
[589,"室外304不锈钢配电箱","1200*600*350mm","最薄处厚度≥1.0mm，挂墙、落地综合","个"]
[590,"配件、耗材"]
[591,"LED控制装置","通用","额定电压AC220V/50HZ","个"]
[592,"电箱指示灯","AC/DC12V","开孔22mm，颜色综合","个"]
[593,"电箱指示灯","AC/DC24V","开孔22mm，颜色综合","个"]
[594,"电箱指示灯","AC220V","开孔22mm，颜色综合","个"]
[595,"电箱指示灯","AC380V","开孔22mm，颜色综合","个"]
[596,"电箱按钮","启动按钮+灯","安装尺寸12-35mm，防护等级:IP40，颜色综合","个"]
[597,"电箱按钮","停止按钮+灯","安装尺寸12-35mm，防护等级:IP40，颜色综合","个"]
[598,"LED模组","12W","三种色温可选：2700K.4000K.6500K","个"]
[599,"底盒修复器","无","可适应于各种底盒","个"]
[600,"铜线鼻子","Φ10","材质：无氧纯铜","个"]
[601,"铜线鼻子","Φ16","材质：无氧纯铜","个"]
[602,"铜线鼻子","Φ25","材质：无氧纯铜","个"]
[603,"铜线鼻子","Φ35","材质：无氧纯铜","个"]
[604,"铜线鼻子","Φ50","材质：无氧纯铜","个"]
[605,"铜线鼻子","Φ70","材质：无氧纯铜","个"]
[606,"铜线鼻子","Φ95","材质：无氧纯铜","个"]
[607,"铜线鼻子","Φ120","材质：无氧纯铜","个"]
[608,"铜线鼻子","Φ150","材质：无氧纯铜","个"]
[609,"管卡","Ø16mm","PVC材质，宽度≥12mm","个"]
[610,"管卡","Ø20mm","PVC材质，宽度≥12mm","个"]
[611,"管卡","Ø25mm","PVC材质，宽度≥12mm","个"]
[612,"管卡","Ø32mm","PVC材质，宽度≥12mm","个"]
[613,"管卡","Ø40mm","PVC材质，宽度≥12mm","个"]
[614,"欧母卡1.5mm厚","Ø16MM","304不锈钢材质","个"]
[615,"欧母卡1.5mm厚","Ø20MM","304不锈钢材质","个"]
[616,"欧母卡1.5mm厚","Ø25MM","304不锈钢材质","个"]
[617,"欧母卡1.5mm厚","Ø32mm","304不锈钢材质","个"]
[618,"欧母卡1.5mm厚","Ø40mm","304不锈钢材质","个"]
[619,"欧母卡0.7mm厚","Ø20MM","304不锈钢材质","个"]
[620,"欧母卡0.7mm厚","Ø25MM","304不锈钢材质","个"]
[621,"欧母卡0.7mm厚","Ø32mm","304不锈钢材质","个"]
[622,"欧母卡0.7mm厚","Ø40mm","304不锈钢材质","个"]
[623,"排卡厚度2mm","Ø16MM","304不锈钢材质，孔数6","个"]
[624,"排卡厚度2mm","Ø20MM","304不锈钢材质，孔数6","个"]
[625,"排卡厚度2mm","Ø25MM","304不锈钢材质，孔数6","个"]
[626,"排卡厚度0.8mm","Ø16MM","304不锈钢材质，孔数6","个"]
[627,"排卡厚度0.8mm","Ø16MM","304不锈钢材质，孔数6","个"]
[628,"排卡厚度0.8mm","Ø16MM","304不锈钢材质，孔数6","个"]
[629,"电工胶布","通用","绝缘性强高粘性电工PVC，宽15mm，层厚≥0.16mm，材质pvc","圈"]
[630,"螺口灯头","通用","适用电压220V,E27螺丝口","个"]
[631,"螺口灯座","通用","适用电压220V,E27螺丝口","个"]
[632,"声光控开关","通用","适用电压220V,E27螺丝口，灵敏度18-45DB","个"]
[633,"绝缘防水胶布","18mm宽，9-10m长，0.13mm厚","生产日期6个月以内","个"]
[634,"地排、零排","11位","黄铜镀镍 ，镀锌螺丝","根"]
[635,"地排、零排","13位","黄铜镀镍 ，镀锌螺丝","根"]
[636,"地排、零排","15位","黄铜镀镍 ，镀锌螺丝","根"]
[637,"地排、零排","17位","黄铜镀镍 ，镀锌螺丝","根"]
[638,"地排、零排","19位","黄铜镀镍 ，镀锌螺丝","根"]
[639,"地排、零排","21位","黄铜镀镍 ，镀锌螺丝","根"]
[640,"电缆热缩套管","(10-16平方)","防水交联绝缘套管","根"]
[641,"电缆热缩套管","(25-50-平方)","防水交联绝缘套管","根"]
[642,"电缆热缩套管","(70-120-平方)","防水交联绝缘套管","根"]
[643,"电缆热缩终端套","(10-16平方)二指套","产品材质交联聚烯烃材质和热熔胶复合","个"]
[644,"电缆热缩终端套","(25-50-平方)二指套","产品材质交联聚烯烃材质和热熔胶复合","个"]
[645,"电缆热缩终端套","(70-120-平方)二指套","产品材质交联聚烯烃材质和热熔胶复合","个"]
[646,"电缆热缩终端套","(10-16平方)三指套","产品材质交联聚烯烃材质和热熔胶复合","个"]
[647,"电缆热缩终端套","(25-50-平方)三指套","产品材质交联聚烯烃材质和热熔胶复合","个"]
[648,"电缆热缩终端套","(70-120-平方)三指套","产品材质交联聚烯烃材质和热熔胶复合","个"]
[649,"电缆热缩终端套","（150-240-平方)三指套","产品材质交联聚烯烃材质和热熔胶复合","个"]
[650,"电缆热缩终端套","(10-16平方)四指套","产品材质交联聚烯烃材质和热熔胶复合","个"]
[651,"电缆热缩终端套","(25-50-平方)四指套","产品材质交联聚烯烃材质和热熔胶复合","个"]
[652,"电缆热缩终端套","(70-120-平方)四指套","产品材质交联聚烯烃材质和热熔胶复合","个"]
[653,"电缆热缩终端套","(10-16平方)五指套","产品材质交联聚烯烃材质和热熔胶复合","个"]
[654,"电缆热缩终端套","(25-50-平方)五指套","产品材质交联聚烯烃材质和热熔胶复合","个"]
[655,"电缆热缩终端套","(70-120-平方)五指套","产品材质交联聚烯烃材质和热熔胶复合","个"]
[656,"3、五金类"]
[657,"铝合金闭门器","轻型","可调速度，定位/不定位综合","个"]
[658,"铝合金闭门器","中型","可调速度，定位/不定位综合","个"]
[659,"铝合金闭门器","重型","可调速度，定位/不定位综合","个"]
[660,"不锈钢顺序器","通用","通用","个"]
[661,"插销","100-125mm","材质：不锈钢","个"]
[662,"插销","175-200mm","材质：不锈钢","个"]
[663,"插销","75-99mm","材质：不锈钢","个"]
[664,"门吸","通用","通用","个"]
[665,"304不锈钢铰链","4寸 弹簧","材质：304不锈钢","个"]
[666,"304不锈钢铰链","5寸 液压","材质：304不锈钢","个"]
[667,"304不锈钢铰链","6寸 液压","材质：304不锈钢","个"]
[668,"304不锈钢铰链","5寸 弹簧","材质：304不锈钢","个"]
[669,"304不锈钢铰链","6寸 弹簧","材质：304不锈钢","个"]
[670,"防盗门锁","通用","适配门厚度：35-50mm，不锈钢材质，钥匙开门，铜锁芯，C级锁芯。","个"]
[671,"老式门外装门锁","通用","钥匙开门，铜锁芯，C级锁芯，冷轧钢锁壳。","个"]
[672,"塑钢门/玻璃门执手锁","通用型","适用于塑钢门，含整套执手、锁体、锁芯，锁芯为铜质，壳体为金属。","个"]
[673,"木门执手锁","通用型","适用于木质套装门，含整套执手、锁体、锁芯，锁芯为铜质，壳体为金属。","个"]
[674,"卷闸门锁","月牙型","材质：合金钢主体  锁芯：铜制","个"]
[675,"卷闸门锁","十字型","材质：合金钢主体  锁芯：铜制","个"]
[676,"卷闸门锁","一字型","材质：合金钢主体  锁芯：铜制","个"]
[677,"挂锁","20cm宽","材质：合金/合金钢/不锈钢/黄铜 ，铜锁芯","个"]
[678,"挂锁","25cm宽","材质：合金/合金钢/不锈钢/黄铜 ，铜锁芯","个"]
[679,"挂锁","30cm宽","材质：合金/合金钢/不锈钢/黄铜 ，铜锁芯","个"]
[680,"挂锁","40cm宽","材质：合金/合金钢/不锈钢/黄铜 ，铜锁芯","个"]
[681,"挂锁","50cm宽","材质：合金/合金钢/不锈钢/黄铜 ，铜锁芯","个"]
[682,"挂锁","60cm宽","材质：合金/合金钢/不锈钢/黄铜 ，铜锁芯","个"]
[683,"挂锁（带密码）","3位","颜色综合，锌合金材质","个"]
[684,"挂锁（带密码）","4位","颜色综合，锌合金材质","个"]
[685,"球形锁","通用型","主体不锈钢，锁芯全铜质","个"]
[686,"铁柜锁","长16-17mm","单开","个"]
[687,"铁柜锁","长20-22mm","单开","个"]
[688,"铁柜锁","长25-27mm","单开","个"]
[689,"铁柜锁","长30-32mm","单开","个"]
[690,"铁柜锁","长40-4mm","单开","个"]
[691,"抽屉锁","16-18mm长","铜锁芯，锌合金面板 单开、通开综合考虑","个"]
[692,"抽屉锁","22-24mm长","主材锌合金锁芯铜","个"]
[693,"U型锁","350-400mm","符合国家标准，满足采购人需求。","个"]
[694,"U型锁（带密码）","350-400mm","符合国家标准，满足采购人需求。","个"]
[695,"不锈钢锁扣","2寸","厚0.7mm","个"]
[696,"不锈钢锁扣","3寸","厚1.0mm","个"]
[697,"不锈钢锁扣","4寸","厚1.0mm","个"]
[698,"消防门锁芯","通用","材质铜质","个"]
[699,"防盗门锁芯","通用","材质铜质，C级锁芯","个"]
[700,"执手门锁芯","通用","材质铜质","个"]
[701,"木门锁芯","通用","材质铜质","个"]
[702,"木质套装门锁体","通用","材质不锈钢/锌合金","个"]
[703,"消防门木门锁体","通用","材质不锈钢/锌合金","个"]
[704,"防盗门锁体","通用型","材质不锈钢/锌合金","个"]
[705,"塑钢门/玻璃门锁体","通用型","材质不锈钢/锌合金","个"]
[706,"铁链条","1米","适用于8-12mm","个"]
[707,"木质套装门把手","通用型","通用型，含面板，不含锁体、锁芯","个"]
[708,"铁皮柜把手","通用型","通用型，含面板，不含锁体、锁芯","个"]
[709,"塑钢门/玻璃门把手","通用型","通用型，含面板，不含锁体、锁芯","个"]
[710,"防火门把手","通用型","通用型，含面板，不含锁体、锁芯","个"]
[711,"防盗门把手","通用型","通用型，含面板，不含锁体、锁芯","个"]
[712,"纱窗按压把手","不锈钢","材质：不锈钢","个"]
[713,"玻璃窗把手","不锈钢","材质：不锈钢","个"]
[714,"柜门拉手","孔距90-100","材质：不锈钢，合金等","个"]
[715,"柜门拉手","孔距190-200","材质：不锈钢，合金等","个"]
[716,"柜门拉手","孔距120-130","材质：不锈钢，合金等","个"]
[717,"玻璃门不锈钢拉手","30-50cm","材质：不锈钢 ","个"]
[718,"玻璃门不锈钢拉手","60-80cm","材质：不锈钢 ","个"]
[719,"不锈钢抽屉轨道","25cm","阻尼三节轨","根"]
[720,"不锈钢抽屉轨道","30cm","阻尼三节轨","根"]
[721,"不锈钢抽屉轨道","35cm","阻尼三节轨","根"]
[722,"不锈钢抽屉轨道","40cm","阻尼三节轨","根"]
[723,"合页","不锈钢","主材不锈钢","个"]
[724,"合页","塑料","主材塑料","个"]
[725,"飞机合页","通用","材质：304不锈钢","个"]
[726,"子母合页","通用","材质：304不锈钢","个"]
[727,"吊梭门滑轮","不锈钢","锌合金+铁+尼龙轮","个"]
[728,"燕尾螺丝","综合","材质：碳钢或者合金钢淬火并回火制成，表面镀锌，符合GB/T3098.1最新标准。","颗"]
[729,"门锁螺丝配件","综合","材质：碳钢或者合金钢淬火并回火制成，表面镀锌，符合GB/T3098.1最新标准。","颗"]
[730,"内/外/燕尾/自攻螺丝","M1*25以内","304不锈钢，符合GB/T3098.6、GB/T3098.15最新标准。","颗"]
[731,"内/外/燕尾/自攻螺丝","M1*50以内","304不锈钢，符合GB/T3098.6、GB/T3098.15最新标准。","颗"]
[732,"内/外/燕尾/自攻螺丝","M2*30以内","304不锈钢，符合GB/T3098.6、GB/T3098.15最新标准。","颗"]
[733,"内/外/燕尾/自攻螺丝","M2*50以内","304不锈钢，符合GB/T3098.6、GB/T3098.15最新标准。","颗"]
[734,"内/外/燕尾/自攻螺丝","M3*90以内","304不锈钢，符合GB/T3098.6、GB/T3098.15最新标准。","颗"]
[735,"内/外/燕尾/自攻螺丝","M4*50以内","304不锈钢，符合GB/T3098.6、GB/T3098.15最新标准。","颗"]
[736,"内/外/燕尾/自攻螺丝","M4*90以内","304不锈钢，符合GB/T3098.6、GB/T3098.15最新标准。","颗"]
[737,"内/外/燕尾/自攻螺丝","M6*50以内","304不锈钢，符合GB/T3098.6、GB/T3098.15最新标准。","颗"]
[738,"内/外/燕尾/自攻螺丝","M6*90以内","304不锈钢，符合GB/T3098.6、GB/T3098.15最新标准。","颗"]
[739,"内/外/燕尾/自攻螺丝","M8*50以内","304不锈钢，符合GB/T3098.6、GB/T3098.15最新标准。","颗"]
[740,"内/外/燕尾/自攻螺丝","M8*90以内","304不锈钢，符合GB/T3098.6、GB/T3098.15最新标准。","颗"]
[741,"内/外/燕尾/自攻螺丝","M10*50以内","304不锈钢，符合GB/T3098.6、GB/T3098.15最新标准。","颗"]
[742,"内/外/燕尾/自攻螺丝","M10*90以内","304不锈钢，符合GB/T3098.6、GB/T3098.15最新标准。","颗"]
[743,"内/外/燕尾/自攻螺丝","M1*25以内","材质：碳钢或者合金钢淬火并回火制成，表面镀锌，符合GB/T3098.1最新标准。","颗"]
[744,"内/外/燕尾/自攻螺丝","M1*50以内","材质：碳钢或者合金钢淬火并回火制成，表面镀锌，符合GB/T3098.1最新标准。","颗"]
[745,"内/外/燕尾/自攻螺丝","M2*30以内","材质：碳钢或者合金钢淬火并回火制成，表面镀锌，符合GB/T3098.1最新标准。","颗"]
[746,"内/外/燕尾/自攻螺丝","M2*50以内","材质：碳钢或者合金钢淬火并回火制成，表面镀锌，符合GB/T3098.1最新标准。","颗"]
[747,"内/外/燕尾/自攻螺丝","M3*90以内","材质：碳钢或者合金钢淬火并回火制成，表面镀锌，符合GB/T3098.1最新标准。","颗"]
[748,"内/外/燕尾/自攻螺丝","M4*50以内","材质：碳钢或者合金钢淬火并回火制成，表面镀锌，符合GB/T3098.1最新标准。","颗"]
[749,"内/外/燕尾/自攻螺丝","M4*90以内","材质：碳钢或者合金钢淬火并回火制成，表面镀锌，符合GB/T3098.1最新标准。","颗"]
[750,"内/外/燕尾/自攻螺丝","M6*50以内","材质：碳钢或者合金钢淬火并回火制成，表面镀锌，符合GB/T3098.1最新标准。","颗"]
[751,"内/外/燕尾/自攻螺丝","M6*90以内","材质：碳钢或者合金钢淬火并回火制成，表面镀锌，符合GB/T3098.1最新标准。","颗"]
[752,"内/外/燕尾/自攻螺丝","M8*50以内","材质：碳钢或者合金钢淬火并回火制成，表面镀锌，符合GB/T3098.1最新标准。","颗"]
[753,"内/外/燕尾/自攻螺丝","M8*90以内","材质：碳钢或者合金钢淬火并回火制成，表面镀锌，符合GB/T3098.1最新标准。","颗"]
[754,"内/外/燕尾/自攻螺丝","M10*50以内","材质：碳钢或者合金钢淬火并回火制成，表面镀锌，符合GB/T3098.1最新标准。","颗"]
[755,"内/外/燕尾/自攻螺丝","M10*90以内","材质：碳钢或者合金钢淬火并回火制成，表面镀锌，符合GB/T3098.1最新标准。","颗"]
[756,"内/外/燕尾/自攻螺丝","M12*50以内","材质：碳钢或者合金钢淬火并回火制成，表面镀锌，符合GB/T3098.1最新标准。","颗"]
[757,"内/外/燕尾/自攻螺丝","M12*100以内","材质：碳钢或者合金钢淬火并回火制成，表面镀锌，符合GB/T3098.1最新标准。","颗"]
[758,"内/外/燕尾/自攻螺丝","M14*50以内","材质：碳钢或者合金钢淬火并回火制成，表面镀锌，符合GB/T3098.1最新标准。","颗"]
[759,"内/外/燕尾/自攻螺丝","M14*100以内","材质：碳钢或者合金钢淬火并回火制成，表面镀锌，符合GB/T3098.1最新标准。","颗"]
[760,"内/外/燕尾/自攻螺丝","M16*50以内","材质：碳钢或者合金钢淬火并回火制成，表面镀锌，符合GB/T3098.1最新标准。","颗"]
[761,"内/外/燕尾/自攻螺丝","M16*100以内","材质：碳钢或者合金钢淬火并回火制成，表面镀锌，符合GB/T3098.1最新标准。","颗"]
[762,"开口塑料膨胀塞","M3*50以内","尼龙材质，颜色，形状综合。","颗"]
[763,"开口塑料膨胀塞","M3*90以内","尼龙材质，颜色，形状综合。","颗"]
[764,"开口塑料膨胀塞","M4*50以内","尼龙材质，颜色，形状综合。","颗"]
[765,"开口塑料膨胀塞","M4*90以内","尼龙材质，颜色，形状综合。","颗"]
[766,"开口塑料膨胀塞","M6*50以内","尼龙材质，颜色，形状综合。","颗"]
[767,"开口塑料膨胀塞","M6*90以内","尼龙材质，颜色，形状综合。","颗"]
[768,"开口塑料膨胀塞","M8*50以内","尼龙材质，颜色，形状综合。","颗"]
[769,"开口塑料膨胀塞","M8*90以内","尼龙材质，颜色，形状综合。","颗"]
[770,"开口塑料膨胀塞","M10*50以内","尼龙材质，颜色，形状综合。","颗"]
[771,"开口塑料膨胀塞","M10*100以内","尼龙材质，颜色，形状综合。","颗"]
[772,"开口塑料膨胀塞","M12*50以内","尼龙材质，颜色，形状综合。","颗"]
[773,"开口塑料膨胀塞","M12*100以内","尼龙材质，颜色，形状综合。","颗"]
[774,"304不锈钢膨胀螺栓","M6*50以内","304不锈钢，形状综合。","颗"]
[775,"304不锈钢膨胀螺栓","M6*90以内","304不锈钢，形状综合。","颗"]
[776,"304不锈钢膨胀螺栓","M8*50以内","304不锈钢，形状综合。","颗"]
[777,"304不锈钢膨胀螺栓","M8*90以内","304不锈钢，形状综合。","颗"]
[778,"304不锈钢膨胀螺栓","M10*50以内","304不锈钢，形状综合。","颗"]
[779,"304不锈钢膨胀螺栓","M10*100以内","304不锈钢，形状综合。","颗"]
[780,"304不锈钢膨胀螺栓","M12*50以内","304不锈钢，形状综合。","颗"]
[781,"304不锈钢膨胀螺栓","M12*100以内","304不锈钢，形状综合。","颗"]
[782,"304不锈钢膨胀螺栓","M14*50以内","304不锈钢，形状综合。","颗"]
[783,"304不锈钢膨胀螺栓","M14*100以内","304不锈钢，形状综合。","颗"]
[784,"304不锈钢膨胀螺栓","M16*50以内","304不锈钢，形状综合。","颗"]
[785,"304不锈钢膨胀螺栓","M16*100以内","304不锈钢，形状综合。","颗"]
[786,"塑料膨胀螺丝","10mm","内置式拉爆沉头","颗"]
[787,"塑料膨胀螺丝","8mm","内置式拉爆沉头","颗"]
[788,"水泥钉","2公分","材质：中碳钢钢钉，符合GB/T 27704-2011最新标准。","kg"]
[789,"水泥钉","4公分","材质：中碳钢钢钉，符合GB/T 27704-2011最新标准。","kg"]
[790,"水泥钉","5公分","材质：中碳钢钢钉","kg"]
[791,"抽芯铆钉","5公分","材质铝帽铁芯，符合国家标准，满足采购人需求。","kg"]
[792,"铁钉","综合","材质铁","kg"]
[793,"钢钉（水泥钉）","1.7*16mm","材质：中碳钢钢钉，符合GB/T 27704-2011最新标准。","颗"]
[794,"钢钉（水泥钉）","2.0*20mm","材质：中碳钢钢钉，符合GB/T 27704-2011最新标准。","颗"]
[795,"钢钉（水泥钉）","2.5*25mm","材质：中碳钢钢钉，符合GB/T 27704-2011最新标准。","颗"]
[796,"钢钉（水泥钉）","2.8*30mm","材质：中碳钢钢钉，符合GB/T 27704-2011最新标准。","颗"]
[797,"钢钉（水泥钉）","3.1*40mm","材质：中碳钢钢钉，符合GB/T 27704-2011最新标准。","颗"]
[798,"钢钉（水泥钉）","3.4*50mm","材质：中碳钢钢钉，符合GB/T 27704-2011最新标准。","颗"]
[799,"线钉","4mm","塑胶材料和中碳钢钢钉","颗"]
[800,"线钉","6mm","塑胶材料和中碳钢钢钉","颗"]
[801,"线钉","8mm","塑胶材料和中碳钢钢钉","颗"]
[802,"线钉","10mm","塑胶材料和中碳钢钢钉","颗"]
[803,"线钉","12mm","塑胶材料和中碳钢钢钉","颗"]
[804,"线钉","4mm","塑胶材料和中碳钢钢钉","颗"]
[805,"盘根","综合","耐磨、耐高温","kg"]
[806,"铁丝","综合","镀锌,q195线材","kg"]
[807,"钢丝","综合","钢丝","kg"]
[808,"不锈钢钢丝","综合","不锈钢钢丝","kg"]
[809,"锁电脑钢丝、带安装","钢丝","主材钢丝","根"]
[810,"不锈钢角码2mm厚","单边20-25mm长","90度直角，配螺丝，孔洞综合","个"]
[811,"不锈钢角码2mm厚","单边30-40mm长","90度直角，配螺丝，孔洞综合","个"]
[812,"不锈钢角码2mm厚","单边40-50mm长","90度直角，配螺丝，孔洞综合","个"]
[813,"不锈钢角码3mm厚","单边20-25mm长","90度直角，配螺丝，孔洞综合","个"]
[814,"不锈钢角码3mm厚","单边30-40mm长","90度直角，配螺丝，孔洞综合","个"]
[815,"不锈钢角码3mm厚","单边40-50mm长","90度直角，配螺丝，孔洞综合","个"]
[816,"不锈钢角码1.5mm厚","单边30-40mm长","90度直角，配螺丝，孔洞综合","个"]
[817,"角钢","∠40*40*3","符合国标","m"]
[818,"304不锈钢抱箍","最大直径6-15mm之间","304不锈钢带手柄喉箍","个"]
[819,"304不锈钢抱箍","最大直径15-25mm之间","304不锈钢带手柄喉箍","个"]
[820,"304不锈钢抱箍","最大直径30-45mm之间","304不锈钢带手柄喉箍","个"]
[821,"304不锈钢抱箍","最大直径45-60mm之间","304不锈钢带手柄喉箍","个"]
[822,"304不锈钢抱箍","最大直径60-80mm之间","304不锈钢带手柄喉箍","个"]
[823,"304不锈钢抱箍","最大直径80-100mm之间","304不锈钢带手柄喉箍","个"]
[824,"304不锈钢抱箍","最大直径100-120mm之间","304不锈钢带手柄喉箍","个"]
[825,"304不锈钢抱箍","最大直径120-150mm之间","304不锈钢带手柄喉箍","个"]
[826,"单挂钩","1钩","防腐防锈优质铝材多层电镀/不锈钢","个"]
[827,"排挂钩","2钩","防腐防锈优质铝材多层电镀/不锈钢","个"]
[828,"排挂钩","3钩","防腐防锈优质铝材多层电镀/不锈钢","个"]
[829,"排挂钩","4钩","防腐防锈优质铝材多层电镀/不锈钢","个"]
[830,"排挂钩","5钩","防腐防锈优质铝材多层电镀/不锈钢","个"]
[831,"排挂钩","6钩","防腐防锈优质铝材多层电镀/不锈钢","个"]
[832,"窗帘挂钩","不锈钢/ 四爪钩","不锈钢","个"]
[833,"末端防虫网","0.3m2尺寸综合","加厚聚乙烯纱网","块"]
[834,"整理线用缠绕管","Ø12mm以内","PE聚乙烯","m"]
[835,"整理线用缠绕管","Ø16mm以内","PE聚乙烯","m"]
[836,"整理线用缠绕管","Ø20mm以内","PE聚乙烯","m"]
[837,"整理线用缠绕管","Ø28mm以内","PE聚乙烯","m"]
[838,"整理线用缠绕管","Ø42mm以内","PE聚乙烯","m"]
[839,"遥控门铃","1按1响","无线安装，可换铃声、可调节音量","个"]
[840,"遥控门铃","2按1响","无线安装，可换铃声、可调节音量","个"]
[841,"遥控门铃","3按1响","无线安装，可换铃声、可调节音量","个"]
[842,"遥控门铃","1按2响","无线安装，可换铃声、可调节音量","个"]
[843,"遥控门铃","2按3响","无线安装，可换铃声、可调节音量","个"]
[844,"遥控门铃","3按2响","无线安装，可换铃声、可调节音量","个"]
[845,"保温壶","容量1.5L","材质不锈钢","个"]
[846,"置物角架","通用","铝合金扇形圆弧","个"]
[847,"置物架","长度30cm 以内","铝合金","个"]
[848,"置物架","长度50cm 以内","铝合金","个"]
[849,"置物架","长度70cm 以内","铝合金","个"]
[850,"浴室隔帘","80cm宽以内","含挂环，高度综合","付"]
[851,"浴室隔帘","100cm宽以内","含挂环，高度综合","付"]
[852,"浴室隔帘","120cm宽以内","含挂环，高度综合","付"]
[853,"浴室隔帘","140cm宽以内","含挂环，高度综合","付"]
[854,"浴室隔帘","160cm宽以内","含挂环，高度综合","付"]
[855,"浴室隔帘杆（XXm）","综合","不锈钢/铝合金综合，打孔，免打孔综合","m"]
[856,"电机","风扇用","材质：纯铜，带双滚珠轴承","个"]
[857,"转向轮","椅子专用","防水防锈耐磨","个"]
[858,"橡胶万向轮","直径10cm以内","推车专用","个"]
[859,"橡胶万向轮","直径12cm以内","推车专用","个"]
[860,"橡胶万向轮","直径15cm以内","推车专用","个"]
[861,"4、维修工具材料"]
[862,"剥线钳","重型","剥线孔径：0.8/1.0/1.6/2.0/2.6㎜","个"]
[863,"瓷砖钻头","616#","材质：金刚砂","个"]
[864,"电工包","长34-35cm、宽15-18cm","三层帆布，配内插孔","个"]
[865,"电工工具腰带","腰带式","帆布","个"]
[866,"电工刀","通用","不锈钢刀身、木柄","个"]
[867,"管钳","8寸","高碳钢材质","个"]
[868,"管钳","10寸","高碳钢材质","个"]
[869,"管钳","12寸","高碳钢材质","个"]
[870,"管钳","14寸","高碳钢材质","个"]
[871,"管钳","18寸","高碳钢材质","个"]
[872,"钳表","交流600A","具有过载保护功能，防止误操作烧坏","个"]
[873,"电笔","感应式","包胶手柄，数显，磁性批头","个"]
[874,"扳手","19#","双头开口：19mm，镜面抛光","个"]
[875,"扳手","17#","双头开口：17mm，镜面抛光","个"]
[876,"扳手","15#","双头开口：15mm，镜面抛光","个"]
[877,"扳手","14#","双头开口：14mm，镜面抛光","个"]
[878,"扳手","12#","双头开口：12mm，镜面抛光","个"]
[879,"扳手","8#","双头开口：8mm，镜面抛光","个"]
[880,"改刀","125#","优质CR-V批头带强磁","个"]
[881,"榔头","SS-010103","高碳钢材质","个"]
[882,"钢丝钳","GS-112","钳身镀烙双色材料手柄","个"]
[883,"尖嘴钳","6寸","钳身镀烙双色材料手柄","个"]
[884,"棘轮扳手","通用","整体长度：150mm","个"]
[885,"手动疏通器","疏通专用","长度：3-3.5m","个"]
[886,"温湿度计","ZW2020","铝质表盘ABS环保外壳","个"]
[887,"推车","600mm*900mm","材质：钢板，耐磨静音轮，承重≥300kg,可折叠车把","个"]
[888,"5、维修耗材"]
[889,"AB胶","10-12g/支","AB胶搭配使用","支"]
[890,"中性硅酮密封胶","300ml","颜色综合，生产日期6个月以内。符合JC/T485最新标准","支"]
[891,"防霉中性硅硅酮密封胶","300ml","颜色综合，生产日期6个月以内。符合JC/T885最新标准","支"]
[892,"硅酮耐候密封胶","300ml","颜色综合，生产日期6个月以内。符合符合最新标准","支"]
[893,"硅酮结构密封胶","590-600ml","颜色综合，生产日期6个月以内。符合GB16776最新标准","支"]
[894,"硅酮结构密封胶","300ml","颜色综合，生产日期6个月以内。符合GB16776最新标准","支"]
[895,"免钉胶","300ml","颜色综合，生产日期6个月以内。符合JC/T 2186最新标准","支"]
[896,"免钉胶","50ml","颜色综合，生产日期6个月以内。符合JC/T 2186最新标准","支"]
[897,"云石胶（XX Kg）","快干型","​​颜色综合，生产日期6个月以内。符合JC/T 989最新标准","kg"]
[898,"云石胶（XX L）","快干型","​​颜色综合，生产日期6个月以内。符合JC/T 989最新标准","L"]
[899,"502胶水","3g","​​颜色综合，生产日期6个月以内。符合HG/T 2492最新标准","支/瓶"]
[900,"502胶水","8g","​​颜色综合，生产日期6个月以内。符合HG/T 2492最新标准","支/瓶"]
[901,"502胶水","15g","​​颜色综合，生产日期6个月以内。符合HG/T 2492最新标准","支/瓶"]
[902,"硬质PVC-U胶粘剂","100ml","​​颜色综合，生产日期6个月以内。符合QB/T 2568最新标准","瓶"]
[903,"氯丁胶（粘得牢）","净重80-90g","​​颜色综合，生产日期6个月以内。","瓶"]
[904,"泡沫胶","750ml","​​颜色综合，生产日期6个月以内。符合T/CPUIA 0001最新标准","支"]
[905,"螺丝松动剂WD-40型","40ml","​​颜色综合，生产日期6个月以内。","瓶"]
[906,"螺丝松动剂WD-40型","100ml","​​颜色综合，生产日期6个月以内。","瓶"]
[907,"螺丝松动剂WD-40型","200ml","​​颜色综合，生产日期6个月以内。","瓶"]
[908,"螺丝松动剂WD-40型","400ml","​​颜色综合，生产日期6个月以内。","瓶"]
[909,"扎带4*200mm","(100条/包）","材质：采用UL认可材料/防火等级94V-2， 规格4*200mm","包"]
[910,"水性调和漆（XX Kg）","桶装","​​颜色综合，生产日期6个月以内。符合GB/23999最新标准","kg"]
[911,"五合一乳胶漆（XX L）","桶装","​​颜色综合，生产日期6个月以内。符合最新标准","L"]
[912,"内墙腻子（XX Kg）","综合","​​颜色综合","kg"]
[913,"外墙腻子（XX Kg）","综合","​​颜色综合","kg"]
[914,"仿瓷涂料","综合","​​颜色综合","kg"]
[915,"喷漆","350ml","​​颜色综合，生产日期6个月以内。","瓶"]
[916,"防火涂料","超薄型","​​颜色综合，生产日期6个月以内。","kg"]
[917,"丹红防锈漆","综合","​​颜色综合，生产日期6个月以内。","kg"]
[918,"丙纶","400g/m2","符合国家标准。","m2"]
[919,"水泥32.5","袋子","符合国家标准。","kg"]
[920,"细沙","综合","符合国家标准。","kg"]
[921,"石粉","综合","符合国家标准。","kg"]
[922,"瓷砖","20*30cm","颜色综合","张"]
[923,"瓷砖","30*30cm  ","颜色综合","张"]
[924,"瓷砖","30*60cm","颜色综合","张"]
[925,"瓷砖","60*60cm","颜色综合","张"]
[926,"瓷砖","40*80cm","颜色综合","张"]
[927,"瓷砖","80*80cm","颜色综合","张"]
[928,"铝塑板","（1220*2440*3）mm","1.产品规格：1220mm*2440mm*3mm，2.产品材质：防火阻燃芯材","张"]
[929,"铝塑板","（1220*2440*4）mm","1.产品规格：1220mm*2440mm*4mm，2.产品材质：防火阻燃芯材","张"]
[930,"石膏板","（1200*2400*9.5）mm","防火等级A2,边角不爆，防开裂","张"]
[931,"木方","3*5cm","符合国家标准。","米"]
[932,"硅钙板/矿棉板","（60*60）cm","符合国家标准。","张"]
[933,"油漆滚筒","9寸","9寸滚筒刷子，羊毛滚芯","个"]
[934,"油漆滚筒","6寸","9寸滚筒刷子，羊毛滚芯","个"]
[935,"油漆刷","100#","不脱毛棕毛","把"]
[936,"油漆刷","25#","不脱毛棕毛","把"]
[937,"油漆刷","50#","不脱毛棕毛","把"]
[938,"电缆封堵防火泥","综合","防火，防水，耐腐蚀，耐油污，阻燃，延展可塑，符合GB23864最新标准","KG"]
[939,"砂轮片","直径105-110mm，厚度1.2mm","符合国家标准。","个"]
[940,"砂纸","168#","碳化硅磨料牛皮纸低基≥120目","张"]
[941,"遮阳网","6针","综合","m2"]
[942,"遮阳网","8针","综合","m2"]
[943,"304不锈钢网","6mm孔.0.6mm丝","长宽综合","m2"]
[944,"花胶布","综合","整张不裁剪","m2"]
[945,"塑料薄膜","厚度12丝","整张不裁剪","m2"]
[946,"塑料薄膜","厚度6丝","整张不裁剪","m2"]
[947,"塑料薄膜","厚度0.8丝","整张不裁剪","m2"]
[948,"推车轮子","推车配件","1.规格：3寸, 脚轮直径60-75mm 轮面宽度28-33mm ,孔距10-12mm，材质：橡胶。","个"]
[949,"美工刀（刀架+刀片）","长150-170mm","合金钢刀片，双排扣刀架","个"]
[950,"美工刀片","宽18-20mm","合金钢材质","盒"]
[951,"6、电器材料"]
[952,"排风扇","开孔（300*300）mm","1.产品外形尺寸36cm*36cm，额定功率40-45W，额定电压220V","个"]
[953,"灭蝇灯","壁挂式","输入电压220V-50HZ，额定功率35W，灯管型号2*10W诱蚊灯管","个"]
[954,"电热水壶","1.7-1.8L","内胆304不锈钢","个"]
[955,"水泵（污水）","120-130W","功率,电压220V,扬程10M","个"]
[956,"集成吊顶换气扇","300mm*300mm","内机机身尺寸300mmx300mmx110mm","个"]
[957,"工业壁扇","综合","电压220V.功率330-350W.档位三档","个"]
[958,"换气扇","吊装 30×30","风量1000-1200m3/h，功率50-70w。","个"]
[959,"防爆型换气扇","防爆型 30×30cm","风量2200-2400m3/h，功率120w-140w。带防爆标志","个"]
[960,"工业级排风扇（轴流风机）","30×30cm","220伏、转速1450r/min 功率120w-140w。带防爆标志","个"]
[961,"专用电动疏通器","2200-2300w","纯铜电机","个"]
[962,"电动疏通器配套钢丝","10mm","钢丝丝径不小于3.5mm","m"]
[963,"电动疏通器配套钢丝","16mm","钢丝丝径不小于3.5mm","m"]
[964,"电动疏通器配套钢丝","22mm","钢丝丝径不小于3.5mm","m"]
[]
[null,"供应商名称（盖章）："]
[null,"联系人及电话："]
[null,"日期："]